VERSION:157

32768,,WLAN_MODULE_INF -  INF_DBGID_DEFINITION_START  
32769,2I,WLAN_MODULE_INF -  INF_ASSERTION_FAILED 0x%x 0x%x
32770,I,WLAN_MODULE_INF -  INF_TARGET_ID 0x%x
32771,4I,WLAN_MODULE_INF -  INF_TARGET_MEM_REMAING 0x%x 0x%x 0x%x 0x%x
32772,4I,WLAN_MODULE_INF -  INF_TARGET_MEM_EXT_REMAING 0x%x 0x%x 0x%x 0x%x
32773,4I,WLAN_MODULE_INF -  INF_TARGET_MEM_ALLOC_TRACK 0x%x 0x%x 0x%x 0x%x
32774,4I,WLAN_MODULE_INF -  INF_TARGET_MEM_ALLOC_RAM 0x%x 0x%x 0x%x 0x%x
32775,,WLAN_MODULE_INF -  INF_DBGID_DEFINITION_END 
33280,,WMI -  WMI_DBGID_DEFINITION_START 
33281,,WMI -  WMI_CMD_RX_XTND_PKT_TOO_SHORT 
33282,,WMI -  WMI_EXTENDED_CMD_NOT_HANDLED 
33283,,WMI -  WMI_CMD_RX_PKT_TOO_SHORT 
33284,,WMI -  WMI_CALLING_WMI_EXTENSION_FN 
33285,I,WMI -  WMI_CMD_NOT_HANDLED CmdId = 0x%x
33286,,WMI -  WMI_IN_SYNC 
33287,,WMI -  WMI_TARGET_WMI_SYNC_CMD 
33288,,WMI -  WMI_SET_SNR_THRESHOLD_PARAMS 
33289,,WMI -  WMI_SET_RSSI_THRESHOLD_PARAMS 
33290,,WMI -  WMI_SET_LQ_TRESHOLD_PARAMS 
33291,,WMI -  WMI_TARGET_CREATE_PSTREAM_CMD 
33292,,WMI -  WMI_WI_DTM_INUSE 
33293,,WMI -  WMI_TARGET_DELETE_PSTREAM_CMD 
33294,,WMI -  WMI_TARGET_IMPLICIT_DELETE_PSTREAM_CMD 
33295,,WMI -  WMI_TARGET_GET_BIT_RATE_CMD 
33296,,WMI -  WMI_GET_RATE_MASK_CMD_FIX_RATE_MASK_IS 
33297,,WMI -  WMI_TARGET_GET_AVAILABLE_CHANNELS_CMD 
33298,,WMI -  WMI_TARGET_GET_TX_PWR_CMD 
33299,,WMI -  WMI_FREE_EVBUF_WMIBUF 
33300,,WMI -  WMI_FREE_EVBUF_DATABUF 
33301,,WMI -  WMI_FREE_EVBUF_BADFLAG 
33302,,WMI -  WMI_HTC_RX_ERROR_DATA_PACKET 
33303,,WMI -  WMI_HTC_RX_SYNC_PAUSING_FOR_MBOX 
33304,,WMI -  WMI_INCORRECT_WMI_DATA_HDR_DROPPING_PKT 
33305,,WMI -  WMI_SENDING_READY_EVENT 
33306,,WMI -  WMI_SETPOWER_MDOE_TO_MAXPERF 
33307,,WMI -  WMI_SETPOWER_MDOE_TO_REC 
33308,,WMI -  WMI_BSSINFO_EVENT_FROM 
33309,,WMI -  WMI_TARGET_GET_STATS_CMD 
33310,,WMI -  WMI_SENDING_SCAN_COMPLETE_EVENT 
33311,,WMI -  WMI_SENDING_RSSI_INDB_THRESHOLD_EVENT 
33312,,WMI -  WMI_SENDING_RSSI_INDBM_THRESHOLD_EVENT 
33313,,WMI -  WMI_SENDING_LINK_QUALITY_THRESHOLD_EVENT 
33314,,WMI -  WMI_SENDING_ERROR_REPORT_EVENT 
33315,,WMI -  WMI_SENDING_CAC_EVENT 
33316,,WMI -  WMI_TARGET_GET_ROAM_TABLE_CMD 
33317,,WMI -  WMI_TARGET_GET_ROAM_DATA_CMD 
33318,,WMI -  WMI_SENDING_GPIO_INTR_EVENT 
33319,,WMI -  WMI_SENDING_GPIO_ACK_EVENT 
33320,,WMI -  WMI_SENDING_GPIO_DATA_EVENT 
33321,2I,WMI -  WMI_CMD_RX CmdId = 0x%x Length = %d
33322,I,WMI -  WMI_CMD_RX_XTND CmdId = 0x%x
33323,3I,WMI -  WMI_EVENT_SEND VdevId/EventId = 0x%x VdevMode = %d EventId = 0x%x
33324,I,WMI -  WMI_EVENT_SEND_XTND 
33325,,WMI -  WMI_CMD_PARAMS_DUMP_START 
33326,,WMI -  WMI_CMD_PARAMS_DUMP_END 
33327,4I,WMI -  WMI_CMD_PARAMS VdevId/AC/Arg1 = %d Cmd/Med-Time/Action/Arg2 = %d DwnGrd_Type = %d Arg4 = %d
33328,2I,WMI -  WMI_EVENT_ALLOC_FAILURE EventId = 0x%x AssocId/VdevMap = 0x%x
33329,,WMI -  WMI_DBGID_DCS_PARAM_CMD 
33330,I,WMI -  WMI_SEND_EVENT_WRONG_TLV CmdId/EventId = 0x%x
33331,,WMI -  WMI_SEND_EVENT_NO_TLV_DEF 
33332,,WMI -  WMI_DBGID_DEFINITION_END 
33792,,STA_PWRSAVE -  PS_STA_DEFINITION_START 
33793,4I,STA_PWRSAVE -  PS_STA_PM_ARB_REQUEST ModuleID = %d Flags = 0x%x LastRequestTime = %d Request = %d
33794,2I,STA_PWRSAVE -  PS_STA_DELIVER_EVENT EventType = %d Statue = %d
33795,5I,STA_PWRSAVE -  PS_STA_PSPOLL_SEQ_DONE QueueTime = %d CompleteTime = %d ResponseTime = %d ResponseDuration = %d ResponseFrameCtrl/QosCtrl = 0x%x
33796,I,STA_PWRSAVE -  PS_STA_COEX_MODE Enable = %d
33797,3I,STA_PWRSAVE -  PS_STA_PSPOLL_ALLOW Allow = %d Flags = 0x%x Time = %d
33798,2I,STA_PWRSAVE -  PS_STA_SET_PARAM Param = %d Value = %d
33799,2I,STA_PWRSAVE -  PS_STA_SPECPOLL_TIMER_STARTED TimeUntilNextBcn = %d WakeUpIntl = %d
33800,,STA_PWRSAVE -  PS_STA_SPECPOLL_TIMER_STOPPED 
33801,I,STA_PWRSAVE -  PS_STA_AVG_CHANNEL_CONGESTION BusyChanRunningAvg = %d
33802,2I,STA_PWRSAVE -  PS_STA_UAPSD_AUTO_TRIG VdevID = %d NumAC = %d
33803,5I,STA_PWRSAVE -  PS_STA_UAPSD_AUTO_TRIG_PER_AC WMM_AC = %d UserPriority = %d SrvIntl = %d SuspIntl = %d DelayIntl = %d
33804,I,STA_PWRSAVE -  PS_STA_WOW_MODE Enable = %d
33805,5I,STA_PWRSAVE -  PS_STA_QPOWER_RESYNC VDevUpCnt = %d IsBTConnected = 0x%x Flags = 0x%x VDevSubMode = 0x%x BitMap = 0x%x
33892,,WLAN_MODULE_STA_PWRSAVE -  Module/message 2/100 
34304,,WLAN_MODULE_WHAL -  WHAL_DBGID_DEFINITION_START 
34305,,WLAN_MODULE_WHAL -  WHAL_ERROR_ANI_CONTROL 
34306,,WLAN_MODULE_WHAL -  WHAL_ERROR_CHIP_TEST1 
34307,,WLAN_MODULE_WHAL -  WHAL_ERROR_CHIP_TEST2 
34308,,WLAN_MODULE_WHAL -  WHAL_ERROR_EEPROM_CHECKSUM 
34309,,WLAN_MODULE_WHAL -  WHAL_ERROR_EEPROM_MACADDR 
34310,,WLAN_MODULE_WHAL -  WHAL_ERROR_INTERRUPT_HIU 
34311,,WLAN_MODULE_WHAL -  WHAL_ERROR_KEYCACHE_RESET 
34312,,WLAN_MODULE_WHAL -  WHAL_ERROR_KEYCACHE_SET 
34313,,WLAN_MODULE_WHAL -  WHAL_ERROR_KEYCACHE_TYPE 
34314,,WLAN_MODULE_WHAL -  WHAL_ERROR_KEYCACHE_TKIPENTRY 
34315,,WLAN_MODULE_WHAL -  WHAL_ERROR_KEYCACHE_WEPLENGTH 
34316,,WLAN_MODULE_WHAL -  WHAL_ERROR_PHY_INVALID_CHANNEL 
34317,,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_AWAKE 
34318,5I,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_SET  0x%x 0x%x 0x%x 0x%x 0x%x
34319,2I,WLAN_MODULE_WHAL -  WHAL_ERROR_RECV_STOPDMA  0x%x 0x%x
34320,2I,WLAN_MODULE_WHAL -  WHAL_ERROR_RECV_STOPPCU  0x%x 0x%x
34321,2I,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_CHANNF1  0x%x 0x%x
34322,,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_CHANNF2 
34323,,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_PM 
34324,I,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_OFFSETCAL  0x%x
34325,,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_RFGRANT 
34326,,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_RXFRAME 
34327,,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_STOPDMA 
34328,I,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_ERRID  0x%x
34329,,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_ADCDCCAL1 
34330,,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_ADCDCCAL2 
34331,I,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_TXIQCAL  0x%x
34332,2I,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_RXIQCAL  0x%x 0x%x
34333,,WLAN_MODULE_WHAL -  WHAL_ERROR_RESET_CARRIERLEAK 
34334,2I,WLAN_MODULE_WHAL -  WHAL_ERROR_XMIT_COMPUTE  0x%x 0x%x
34335,,WLAN_MODULE_WHAL -  WHAL_ERROR_XMIT_NOQUEUE 
34336,I,WLAN_MODULE_WHAL -  WHAL_ERROR_XMIT_ACTIVEQUEUE  0x%x
34337,I,WLAN_MODULE_WHAL -  WHAL_ERROR_XMIT_BADTYPE  0x%x
34338,2I,WLAN_MODULE_WHAL -  WHAL_ERROR_XMIT_STOPDMA  0x%x 0x%x
34339,,WLAN_MODULE_WHAL -  WHAL_ERROR_INTERRUPT_BB_PANIC 
34340,,WLAN_MODULE_WHAL -  WHAL_ERROR_PAPRD_MAXGAIN_ABOVE_WINDOW 
34341,2I,WLAN_MODULE_WHAL -  WHAL_ERROR_QCU_HW_PAUSE_MISMATCH  0x%x 0x%x
34342,2I,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_RFLP_CONFIG  0x%x 0x%x
34343,2I,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_RFLP_SYNTHBYPASS_CONFIG  0x%x 0x%x
34344,2I,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_RFLP_BIAS2X_CONFIG  0x%x 0x%x
34345,I,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_RFLP_PLLBYPASS_CONFIG  0x%x
34346,2I,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_RFLP_OFF1CHAN_CONFIG  0x%x 0x%x
34347,,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_ANTENNA_LMIT 
34348,,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_REGDMN_TX_LMIT 
34349,,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_MODE_SCALED_PWR 
34350,,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_EDGE_PWR_TPSCALE 
34351,,WLAN_MODULE_WHAL -  WHAL_ERROR_POWER_CHAN_REGALLOW 
34352,,WLAN_MODULE_WHAL -  WHAL_ERROR_WAIT_REG_TIMEOUT 
34353,,WLAN_MODULE_WHAL -  WHAL_ERROR_XTAL_SET 
34354,,WLAN_MODULE_WHAL -  WHAL_DBGID_DEFINITION_END 
34356,,WLAN_MODULE_WHAL -  Module/message 3/52
34357,,WLAN_MODULE_WHAL -  Module/message 3/53
34358,,WLAN_MODULE_WHAL -  Module/message 3/54 
34359,,WLAN_MODULE_WHAL -  Module/message 3/55 
34360,,WLAN_MODULE_WHAL -  Module/message 3/56 
34366,,WLAN_MODULE_WHAL -  MOdule/message 3/62
34816,,BTCOEX -  COEX_DEBUGID_START 
34817,5I,BTCOEX -  BTCOEX_DBG_MCI_1  %u %u %u %u %u
34818,5I,BTCOEX -  BTCOEX_DBG_MCI_2  %u %u %u %u %u
34819,5I,BTCOEX -  BTCOEX_DBG_MCI_3  %u %u %u %u %u
34820,5I,BTCOEX -  BTCOEX_DBG_MCI_4  %u %u %u %u %u
34821,5I,BTCOEX -  BTCOEX_DBG_MCI_5  %u %u %u %u %u
34822,5I,BTCOEX -  BTCOEX_DBG_MCI_6  %u %u %u %u %u
34823,5I,BTCOEX -  BTCOEX_DBG_MCI_7  %u %u %u %u %u
34824,5I,BTCOEX -  BTCOEX_DBG_MCI_8  %u %u %u %u %u
34825,5I,BTCOEX -  BTCOEX_DBG_MCI_9  %u %u %u %u %u
34826,5I,BTCOEX -  BTCOEX_DBG_MCI_10  0x%x 0x%x 0x%x 0x%x 0x%x
34827,2I,BTCOEX -  COEX_WAL_BTCOEX_INIT  MajorVer=%u MinorVer=%u
34828,2I,BTCOEX -  COEX_WAL_PAUSE  IsPause=%u PauseState=%u
34829,2I,BTCOEX -  COEX_WAL_RESUME  IsPause=%u PauseState=%u
34830,4I,BTCOEX -  COEX_UPDATE_AFH  IsAdd=%u mhz=%u Is2G=%u IsHT20=%u
34831,I,BTCOEX -  COEX_HWQ_EMPTY_CB  PauseState=%u
34832,I,BTCOEX -  COEX_MCI_TIMER_HANDLER  BusRecoveryState=%u
34833,2I,BTCOEX -  COEX_MCI_RECOVER  StimulusState=%u BusRecoveryState=%u
34834,3I,BTCOEX -  ERROR_COEX_MCI_ISR  0x%x 0x%x 0x%x
34835,2I,BTCOEX -  ERROR_COEX_MCI_GPM  SWGpmIndex=%u NumGPMs=%u
34836,I,BTCOEX -  COEX_ProfileType  %u
34837,4I,BTCOEX -  COEX_LinkID  %u %u %u %u
34838,I,BTCOEX -  COEX_LinkState  %u
34839,I,BTCOEX -  COEX_LinkRole  %u
34840,I,BTCOEX -  COEX_LinkRate  %u
34841,I,BTCOEX -  COEX_VoiceType  %u
34842,I,BTCOEX -  COEX_Tinterval  %u
34843,I,BTCOEX -  COEX_Wretrx  %u
34844,I,BTCOEX -  COEX_Attempts  %u
34845,2I,BTCOEX -  COEX_PerformanceState  State=%u OpType=%u
34846,I,BTCOEX -  COEX_LinkType  %u
34847,,BTCOEX -  COEX_RX_MCI_GPM_VERSION_QUERY 
34848,2I,BTCOEX -  COEX_RX_MCI_GPM_VERSION_RESPONSE  MajorVer=%u MinorVer=%u
34849,I,BTCOEX -  COEX_RX_MCI_GPM_STATUS_QUERY  %u
34850,4I,BTCOEX -  COEX_STATE_WLAN_VDEV_DOWN  id=%u CurVdevState=%u NumOfConnectedVdev=%u Stimulus=%u
34851,5I,BTCOEX -  COEX_STATE_WLAN_VDEV_START  id=%u CurVdevState=%u OperatingChannel=%u OpMode=%u SubOpMode=%u
34852,5I,BTCOEX -  COEX_STATE_WLAN_VDEV_CONNECTED  id=%u VdevType=%u PeerSecurityState=%u OpMode=%u SubOpMode=%u
34853,4I,BTCOEX -  COEX_STATE_WLAN_VDEV_SCAN_STARTED  id=%u CurVdevState=%u ScanType=%u IsStrictDuration=%u
34854,3I,BTCOEX -  COEX_STATE_WLAN_VDEV_SCAN_END  id=%u CurVdevState=%u ScanType=%u
34855,2I,BTCOEX -  COEX_STATE_WLAN_DEFAULT  id=%u CurVdevState=%u
34856,5I,BTCOEX -  COEX_CHANNEL_CHANGE  %uMhz->%uMhz WlanSysState=0x%x CurrBand=%u PhyMode=%u
34857,3I,BTCOEX -  COEX_POWER_CHANGE  Event=0x%x PowerState=(%u->%u)
34858,2I,BTCOEX -  COEX_CONFIG_MGR  ConfigManager=%u Stimulus=%u
34859,3I,BTCOEX -  COEX_TX_MCI_GPM_BT_CAL_REQ  Len=%u QFlags=0x%x IsMciHWBusy=%u
34860,3I,BTCOEX -  COEX_TX_MCI_GPM_BT_CAL_GRANT  Len=%u QFlags=0x%x IsMciHWBusy=%u
34861,3I,BTCOEX -  COEX_TX_MCI_GPM_BT_CAL_DONE  Len=%u QFlags=0x%x IsMciHWBusy=%u
34862,3I,BTCOEX -  COEX_TX_MCI_GPM_WLAN_CAL_REQ  Len=%u QFlags=0x%x IsMciHWBusy=%u
34863,3I,BTCOEX -  COEX_TX_MCI_GPM_WLAN_CAL_GRANT  Len=%u QFlags=0x%x IsMciHWBusy=%u
34864,3I,BTCOEX -  COEX_TX_MCI_GPM_WLAN_CAL_DONE  Len=%u QFlags=0x%x IsMciHWBusy=%u
34865,3I,BTCOEX -  COEX_TX_MCI_GPM_BT_DEBUG  Len=%u QFlags=0x%x IsMciHWBusy=%u
34866,3I,BTCOEX -  COEX_TX_MCI_GPM_VERSION_QUERY  Len=%u QFlags=0x%x IsMciHWBusy=%u
34867,3I,BTCOEX -  COEX_TX_MCI_GPM_VERSION_RESPONSE  Len=%u QFlags=0x%x IsMciHWBusy=%u
34868,3I,BTCOEX -  COEX_TX_MCI_GPM_STATUS_QUERY  Len=%u QFlags=0x%x IsMciHWBusy=%u
34869,3I,BTCOEX -  COEX_TX_MCI_GPM_HALT_BT_GPM  Len=%u QFlags=0x%x IsMciHWBusy=%u
34870,3I,BTCOEX -  COEX_TX_MCI_GPM_WLAN_CHANNELS  Len=%u QFlags=0x%x IsMciHWBusy=%u
34871,3I,BTCOEX -  COEX_TX_MCI_GPM_BT_PROFILE_INFO  Len=%u QFlags=0x%x IsMciHWBusy=%u
34872,3I,BTCOEX -  COEX_TX_MCI_GPM_BT_STATUS_UPDATE  Len=%u QFlags=0x%x IsMciHWBusy=%u
34873,3I,BTCOEX -  COEX_TX_MCI_GPM_BT_UPDATE_FLAGS  Len=%u QFlags=0x%x IsMciHWBusy=%u
34874,3I,BTCOEX -  COEX_TX_MCI_GPM_UNKNOWN  Len=%u QFlags=0x%x IsMciHWBusy=%u
34875,3I,BTCOEX -  COEX_TX_MCI_SYS_WAKING  Len=%u QFlags=0x%x IsMciHWBusy=%u
34876,3I,BTCOEX -  COEX_TX_MCI_LNA_TAKE  Len=%u QFlags=0x%x IsMciHWBusy=%u
34877,3I,BTCOEX -  COEX_TX_MCI_LNA_TRANS  Len=%u QFlags=0x%x IsMciHWBusy=%u
34878,3I,BTCOEX -  COEX_TX_MCI_SYS_SLEEPING  Len=%u QFlags=0x%x IsMciHWBusy=%u
34879,3I,BTCOEX -  COEX_TX_MCI_REQ_WAKE  Len=%u QFlags=0x%x IsMciHWBusy=%u
34880,3I,BTCOEX -  COEX_TX_MCI_REMOTE_RESET  Len=%u QFlags=0x%x IsMciHWBusy=%u
34881,3I,BTCOEX -  COEX_TX_MCI_TYPE_UNKNOWN  Len=%u QFlags=0x%x IsMciHWBusy=%u
34882,3I,BTCOEX -  COEX_WHAL_MCI_RESET  Is2G=%u 0x%x 0x%x
34883,,BTCOEX -  COEX_POLL_BT_CAL_DONE_TIMEOUT 
34884,3I,BTCOEX -  COEX_WHAL_PAUSE  WlanCalState=%u WlanMciState=%u BtCalHwPaused=%u
34885,I,BTCOEX -  COEX_RX_MCI_GPM_BT_CAL_REQ  0x%x
34886,,BTCOEX -  COEX_RX_MCI_GPM_BT_CAL_DONE 
34887,2I,BTCOEX -  COEX_RX_MCI_GPM_BT_CAL_GRANT  WlanCalState=%u BtCalState=%u
34888,4I,BTCOEX -  COEX_WLAN_CAL_START  0x%x 0x%x 0x%x 0x%x
34889,,BTCOEX -  COEX_WLAN_CAL_RESULT 
34890,I,BTCOEX -  COEX_BtMciState  0x%x
34891,I,BTCOEX -  COEX_BtCalState  0x%x
34892,I,BTCOEX -  COEX_WlanCalState  0x%x
34893,I,BTCOEX -  COEX_RxReqWakeCount  %u
34894,I,BTCOEX -  COEX_RxRemoteResetCount  %u
34895,,BTCOEX -  COEX_RESTART_CAL 
34896,5I,BTCOEX -  COEX_SENDMSG_QUEUE  MciType=0x%x IsMCIBusPaused=%u PendingMciMsg=0x%x SleepOverride=%u Temp=0x%x
34897,,BTCOEX -  COEX_RESETSEQ_LNAINFO_TIMEOUT 
34898,I,BTCOEX -  COEX_MCI_ISR_IntRaw  0x%x 
34899,I,BTCOEX -  COEX_MCI_ISR_Int1Raw  0x%x  
34900,I,BTCOEX -  COEX_MCI_ISR_RxMsgRaw  0x%x 
34901,4I,BTCOEX -  COEX_WHAL_COEX_RESET  Is2G=%u pWlanConfigManager=0x%x ResetCause=%u IsMciHWBusy=%u
34902,2I,BTCOEX -  COEX_WAL_COEX_INIT  IsChan2G=%u NumOfVdev=%u
34903,2I,BTCOEX -  COEX_TXRX_CNT_LIMIT_ISR  Tx=%u Rx=%u
34904,,BTCOEX -  COEX_CH_BUSY 
34905,2I,BTCOEX -  COEX_REASSESS_WLAN_STATE  WlanSystemState=0x%x PrevWlanSystemState=0x%x
34906,,BTCOEX -  COEX_BTCOEX_WLAN_STATE_UPDATE 
34907,I,BTCOEX -  COEX_BT_NUM_OF_PROFILES  %u
34908,I,BTCOEX -  COEX_BT_NUM_OF_HID_PROFILES  %u
34909,I,BTCOEX -  COEX_BT_NUM_OF_ACL_PROFILES  %u
34910,I,BTCOEX -  COEX_BT_NUM_OF_HI_ACL_PROFILES  %u
34911,I,BTCOEX -  COEX_BT_NUM_OF_VOICE_PROFILES  %u
34912,2I,BTCOEX -  COEX_WLAN_AGGR_LIMIT  vdev_id=%u Aggr_limit=%u
34913,I,BTCOEX -  COEX_BT_LOW_PRIO_BUDGET  %u
34914,I,BTCOEX -  COEX_BT_HI_PRIO_BUDGET  %u
34915,I,BTCOEX -  COEX_BT_IDLE_TIME  %u
34916,5I,BTCOEX -  COEX_SET_COEX_WEIGHT  CurWeightGroup=%u WlanIsIdleOverride=%u QcuWeight=%u WeightOption=%u WlanCoexWeight[0]=%u
34917,I,BTCOEX -  COEX_WLAN_WEIGHT_GROUP  %u 
34918,I,BTCOEX -  COEX_BT_WEIGHT_GROUP  %u
34919,2I,BTCOEX -  COEX_BT_INTERVAL_ALLOC  %u %u
34920,I,BTCOEX -  COEX_BT_SCHEME  0x%x
34921,4I,BTCOEX -  COEX_BT_MGR  Stimulus=%u BtCoexSMState=%u SystemUpdateResult=%u WlanConfigManager=0x%x
34922,2I,BTCOEX -  COEX_BT_SM_ERROR  BtCoexSMState=%u Stimulus=%u
34923,5I,BTCOEX -  COEX_SYSTEM_UPDATE  ReturnStatus=%u WlanSystemState=0x%x TrafficAlgo=%u NumOfWlanRfChains=%u AggrLimit=%u
34924,I,BTCOEX -  COEX_LOW_PRIO_LIMIT  %u
34925,I,BTCOEX -  COEX_HI_PRIO_LIMIT  %u
34926,5I,BTCOEX -  COEX_BT_INTERVAL_START  BtIntvlCnt=%u Duration=%u Weight=%u BaseIdleOverride=%u WeightMat[0]=0x%x
34927,5I,BTCOEX -  COEX_WLAN_INTERVAL_START  WlanIntvlCnt=%u Duration=%u Weight=%u BaseIdleOverride=%u WeightMat[0]=0x%x
34928,I,BTCOEX -  COEX_NON_LINK_BUDGET  %u
34929,2I,BTCOEX -  COEX_CONTENTION_MSG  0x%x 0x%x
34930,2I,BTCOEX -  COEX_SET_NSS  0x%x 0x%x
34931,4I,BTCOEX -  COEX_SELF_GEN_MASK  0x%x 0x%x 0x%x 0x%x
34932,4I,BTCOEX -  COEX_PROFILE_ERROR  0x%x 0x%x 0x%x 0x%x
34933,,BTCOEX -  COEX_WLAN_INIT 
34934,I,BTCOEX -  COEX_BEACON_MISS  BcnRxProtectOverride=%u
34935,I,BTCOEX -  COEX_BEACON_OK  BcnRxProtectOverride=%u
34936,5I,BTCOEX -  COEX_BTCOEX_SCAN_ACTIVITY  0x%x 0x%x 0x%x 0x%x 0x%x
34937,5I,BTCOEX -  COEX_SCAN_ACTIVITY  0x%x 0x%x 0x%x 0x%x 0x%x
34938,I,BTCOEX -  COEX_FORCE_QUIETTIME  0x%x
34939,I,BTCOEX -  COEX_BT_MGR_QUIETTIME  0x%x
34940,I,BTCOEX -  COEX_BT_INACTIVITY_TRIGGER  0x%x
34941,2I,BTCOEX -  COEX_BT_INACTIVITY_REPORTED  BtCoexSMState=%u BtIntervalCnt=%u
34942,3I,BTCOEX -  COEX_TX_MCI_GPM_WLAN_PRIO  Len=%u QFlags=0x%x IsMciHWBusy=%u
34943,3I,BTCOEX -  COEX_TX_MCI_GPM_BT_PAUSE_PROFILE  Len=%u QFlags=0x%x IsMciHWBusy=%u
34944,3I,BTCOEX -  COEX_TX_MCI_GPM_WLAN_SET_ACL_INACTIVITY  Len=%u QFlags=0x%x IsMciHWBusy=%u
34945,I,BTCOEX -  COEX_RX_MCI_GPM_BT_ACL_INACTIVITY_REPORT  Len=%u QFlags=0x%x IsMciHWBusy=%u
34946,5I,BTCOEX -  COEX_GENERIC_ERROR  0x%x 0x%x 0x%x 0x%x 0x%x
34947,5I,BTCOEX -  COEX_RX_RATE_THRESHOLD  0x%x 0x%x 0x%x 0x%x 0x%x
34948,5I,BTCOEX -  COEX_RSSI  0x%x 0x%x 0x%x 0x%x 0x%x
34949,3I,BTCOEX -  COEX_WLAN_VDEV_NOTIF_START  Channel=%u Opmode=%u SubOpmode=%u
34950,3I,BTCOEX -  COEX_WLAN_VDEV_NOTIF_UP  Channel=%u Opmode=%u SubOpmode=%u
34951,I,BTCOEX -  COEX_WLAN_VDEV_NOTIF_DOWN  Channel=%u
34952,,BTCOEX -  COEX_WLAN_VDEV_NOTIF_STOP 
34953,I,BTCOEX -  COEX_WLAN_VDEV_NOTIF_ADD_PEER  Peer=0x%x
34954,3I,BTCOEX -  COEX_WLAN_VDEV_NOTIF_DELETE_PEER  Phymode=%u numOf11bPeers=%u numOf11gPeers=%u
34955,2I,BTCOEX -  COEX_WLAN_VDEV_NOTIF_CONNECTED_PEER  numOf11bPeers=%u numOf11gPeers=%u
34956,I,BTCOEX -  COEX_WLAN_VDEV_NOTIF_PAUSE  0x%x
34957,I,BTCOEX -  COEX_WLAN_VDEV_NOTIF_UNPAUSED  0x%x
34958,3I,BTCOEX -  COEX_STATE_WLAN_VDEV_PEER_ADD  0x%x 0x%x 0x%x
34959,4I,BTCOEX -  COEX_STATE_WLAN_VDEV_CONNECTED_PEER  NumberOfConnectedVdev=%u NumberOfConnectedPeers=%u PeerSecurityState=0x%x NumberOf11gPeers=%u
34960,2I,BTCOEX -  COEX_STATE_WLAN_VDEV_DELETE_PEER  NumberOfConnectedPeers=%u NumberOf11gPeers=%u
34961,2I,BTCOEX -  COEX_STATE_WLAN_VDEV_PAUSE  VdevId=%u CurrentVdevState=0x%x
34962,2I,BTCOEX -  COEX_STATE_WLAN_VDEV_UNPAUSED  VdevId=%u CurrentVdevState=0x%x
34963,2I,BTCOEX -  COEX_SCAN_CALLBACK ScanType=%u VdevId=%u
34964,2I,BTCOEX -  COEX_RC_SET_CHAINMASK  SharedAntennaIndex=%u NumberOfWlanRfChains=%u
34965,3I,BTCOEX -  COEX_TX_MCI_GPM_WLAN_SET_BT_RXSS_THRES  Len=%u QFlags=0x%x IsMciHWBusy=%u
34966,3I,BTCOEX -  COEX_TX_MCI_GPM_BT_RXSS_THRES_QUERY  Len=%u QFlags=0x%x IsMciHWBusy=%u
34967,3I,BTCOEX -  COEX_BT_RXSS_THRES  0x%x NewRSSI=%u BtRxssLowerThreshold=%u
34968,3I,BTCOEX -  COEX_BT_PROFILE_ADD_RMV  %u LinkID=%u ProfileType=%u
34969,,BTCOEX -  COEX_BT_SCHED_INFO 
34970,,BTCOEX -  COEX_TRF_MGMT 
34971,5I,BTCOEX -  COEX_SCHED_START  SchedReq=%u Duration=%u TrafficMgmtAlg=%u WlanRxState=%u RssiType=%u
34972,5I,BTCOEX -  COEX_SCHED_RESULT  SchedReq=%u TrafficMgmtAlg=%u PrevCoexAlg=%u MgrPolicy=0x%x WlanIsIdleOverride=%u
34973,,BTCOEX -  COEX_SCHED_ERROR 
34974,,BTCOEX -  COEX_SCHED_PRE_OP 
34975,,BTCOEX -  COEX_SCHED_POST_OP 
34976,5I,BTCOEX -  COEX_RX_RATE NumOfRxUnderThreshPeers=%u MinDirectRxRate=%u LastRxRateSample=%u DeltaTime=%u last_event=0x%x
34977,,BTCOEX -  COEX_ACK_PRIORITY 
34978,,BTCOEX -  COEX_STATE_WLAN_VDEV_UP
34979,,BTCOEX -  COEX_STATE_WLAN_VDEV_PEER_UPDATE 
34980,,BTCOEX -  COEX_STATE_WLAN_VDEV_STOP 
34981,,BTCOEX -  COEX_WLAN_PAUSE_PEER 
34982,,BTCOEX -  COEX_WLAN_UNPAUSE_PEER 
34983,,BTCOEX -  COEX_WLAN_PAUSE_INTERVAL_START 
34984,2I,BTCOEX -  COEX_WLAN_POSTPAUSE_INTERVAL_START  0x%x 0x%x
34985,5I,BTCOEX -  COEX_TRF_FREERUN  0x%x 0x%x 0x%x 0x%x 0x%x
34986,5I,BTCOEX -  COEX_TRF_SHAPE_PM  0x%x 0x%x 0x%x 0x%x 0x%x
34987,5I,BTCOEX -  COEX_TRF_SHAPE_PSP  0x%x 0x%x 0x%x 0x%x 0x%x
34988,,BTCOEX -  COEX_TRF_SHAPE_S_CTS 
34989,3I,BTCOEX -  COEX_CHAIN_CONFIG  0x%x 0x%x 0x%x
34990,5I,BTCOEX -  COEX_SYSTEM_MONITOR  0x%x 0x%x 0x%x 0x%x 0x%x
34991,,BTCOEX -  COEX_SINGLECHAIN_INIT 
34992,,BTCOEX -  COEX_MULTICHAIN_INIT 
34993,5I,BTCOEX -  COEX_SINGLECHAIN_DBG_1  0x%x 0x%x 0x%x 0x%x 0x%x
34994,5I,BTCOEX -  COEX_SINGLECHAIN_DBG_2  0x%x 0x%x 0x%x 0x%x 0x%x
34995,5I,BTCOEX -  COEX_SINGLECHAIN_DBG_3  0x%x 0x%x 0x%x 0x%x 0x%x
34996,5I,BTCOEX -  COEX_MULTICHAIN_DBG_1  0x%x 0x%x 0x%x 0x%x 0x%x
34997,5I,BTCOEX -  COEX_MULTICHAIN_DBG_2  0x%x 0x%x 0x%x 0x%x 0x%x
34998,5I,BTCOEX -  COEX_MULTICHAIN_DBG_3  0x%x 0x%x 0x%x 0x%x 0x%x
34999,,BTCOEX -  COEX_PSP_TX_CB 
35000,,BTCOEX -  COEX_PSP_RX_CB 
35001,5I,BTCOEX -  COEX_PSP_STAT_1  0x%x 0x%x 0x%x 0x%x 0x%x
35002,5I,BTCOEX -  COEX_PSP_SPEC_POLL  0x%x 0x%x 0x%x 0x%x 0x%x
35003,5I,BTCOEX -  COEX_PSP_READY_STATE  0x%x 0x%x 0x%x 0x%x 0x%x
35004,,BTCOEX -  COEX_PSP_TX_STATUS_STATE 
35005,5I,BTCOEX -  COEX_PSP_RX_STATUS_STATE_1  0x%x 0x%x 0x%x 0x%x 0x%x
35006,,BTCOEX -  COEX_PSP_NOT_READY_STATE 
35007,,BTCOEX -  COEX_PSP_DISABLED_STATE 
35008,,BTCOEX -  COEX_PSP_ENABLED_STATE 
35009,3I,BTCOEX -  COEX_PSP_SEND_PSPOLL  0x%x 0x%x 0x%x
35010,,BTCOEX -  COEX_PSP_MGR_ENTER 
35011,,BTCOEX -  COEX_PSP_MGR_RESULT 
35012,4I,BTCOEX -  COEX_PSP_NONWLAN_INTERVAL  0x%x 0x%x 0x%x 0x%x
35013,5I,BTCOEX -  COEX_PSP_STAT_2  0x%x 0x%x 0x%x 0x%x 0x%x
35014,,BTCOEX -  COEX_PSP_RX_STATUS_STATE_2 
35015,3I,BTCOEX -  COEX_PSP_ERROR  0x%x 0x%x 0x%x
35016,5I,BTCOEX -  COEX_T2BT 0x%x 0x%x 0x%x 0x%x 0x%x
35017,5I,BTCOEX -  COEX_BT_DURATION 0x%x 0x%x 0x%x 0x%x 0x%x
35018,3I,BTCOEX -  COEX_TX_MCI_GPM_WLAN_SCHED_INFO_TRIG  0x%x 0x%x 0x%x
35019,3I,BTCOEX -  COEX_TX_MCI_GPM_WLAN_SCHED_INFO_TRIG_RSP  0x%x 0x%x 0x%x
35020,3I,BTCOEX -  COEX_TX_MCI_GPM_SCAN_OP  0x%x 0x%x 0x%x
35021,,BTCOEX -  COEX_TX_MCI_GPM_BT_PAUSE_GPM_TX 
35022,3I,BTCOEX -  COEX_CTS2S_SEND  0x%x 0x%x 0x%x
35023,I,BTCOEX -  COEX_CTS2S_RESULT  0x%x
35024,4I,BTCOEX -  COEX_ENTER_OCS  0x%x 0x%x 0x%x 0x%x
35025,2I,BTCOEX -  COEX_EXIT_OCS  0x%x 0x%x
35026,4I,BTCOEX -  COEX_UPDATE_OCS  0x%x 0x%x 0x%x 0x%x
35027,5I,BTCOEX -  COEX_STATUS_OCS  0x%x 0x%x 0x%x 0x%x 0x%x
35028,5I,BTCOEX -  COEX_STATS_BT 0x%x 0x%x 0x%x 0x%x 0x%x
35029,,LTECOEX -  COEX_MWS_WLAN_INIT 
35030,3I,LTECOEX -  COEX_MWS_WBTMR_SYNC  0x%x 0x%x 0x%x
35031,,LTECOEX -  COEX_MWS_TYPE2_RX 
35032,,LTECOEX -  COEX_MWS_TYPE2_TX 
35033,5I,LTECOEX -  COEX_MWS_WLAN_CHAVD  0x%x 0x%x 0x%x 0x%x 0x%x
35034,,LTECOEX -  COEX_MWS_WLAN_CHAVD_INSERT 
35035,,LTECOEX -  COEX_MWS_WLAN_CHAVD_MERGE 
35036,3I,LTECOEX -  COEX_MWS_WLAN_CHAVD_RPT  0x%x 0x%x 0x%x
35037,I,LTECOEX -  COEX_MWS_CP_MSG_SEND  frame_size = %u
35038,,LTECOEX -  COEX_MWS_CP_ESCAPE 
35039,I,LTECOEX -  COEX_MWS_CP_UNFRAME  retval = %u
35040,2I,LTECOEX -  COEX_MWS_CP_SYNC_UPDATE  LteState = 0x%x 0x%x
35041,3I,LTECOEX -  COEX_MWS_CP_SYNC  LteState = 0x%x type = 0x%x %u
35042,2I,LTECOEX -  COEX_MWS_CP_WLAN_STATE_IND  LteState = 0x%x WlanToken = 0x%x
35043,,LTECOEX -  COEX_MWS_CP_SYNCRESP_TIMEOUT 
35044,4I,LTECOEX -  COEX_MWS_SCHEME_UPDATE  stimulus online PhyExist LteState = 0x%x PwrLimit LTECycle = 0x%x offset syncState Scheme = 0x%x WlanFreq = %u
35045,3I,LTECOEX -  COEX_MWS_WLAN_EVENT  stimulus = 0x%x inc_token = %u WlanToken = 0x%x
35046,,LTECOEX -  COEX_MWS_UART_UNESCAPE 
35047,4I,LTECOEX -  COEX_MWS_UART_ENCODE_SEND  0x%x 0x%x 0x%x 0x%x
35048,,LTECOEX -  COEX_MWS_UART_RECV_DECODE 
35049,,LTECOEX -  COEX_MWS_UL_HDL 
35050,5I,LTECOEX -  COEX_MWS_REMOTE_EVENT  0x%x 0x%x 0x%x 0x%x 0x%x
35051,5I,LTECOEX -  COEX_MWS_OTHER  0x%x 0x%x 0x%x 0x%x 0x%x
35052,,LTECOEX -  COEX_MWS_ERROR 
35053,5I,LTECOEX -  COEX_MWS_ANT_DIVERSITY  0x%x 0x%x 0x%x 0x%x 0x%x
35054,5I,BTCOEX -  COEX_P2P_GO 0x%x 0x%x 0x%x 0x%x 0x%x
35055,5I,BTCOEX -  COEX_P2P_CLIENT 0x%x 0x%x 0x%x 0x%x 0x%x
35056,5I,BTCOEX -  COEX_SCC_1 0x%x 0x%x 0x%x 0x%x 0x%x
35057,5I,BTCOEX -  COEX_SCC_2 0x%x 0x%x 0x%x 0x%x 0x%x
35058,5I,BTCOEX -  COEX_MCC_1 0x%x 0x%x 0x%x 0x%x 0x%x
35059,5I,BTCOEX -  COEX_MCC_2 0x%x 0x%x 0x%x 0x%x 0x%x
35060,5I,BTCOEX -  COEX_TRF_SHAPE_NOA 
35061,5I,BTCOEX -  COEX_NOA_ONESHOT 
35062,5I,BTCOEX -  COEX_NOA_PERIODIC 
35063,5I,BTCOEX -  COEX_LE_1 0x%x 0x%x 0x%x 0x%x 0x%x
35064,5I,BTCOEX -  COEX_LE_2 0x%x 0x%x 0x%x 0x%x 0x%x
35065,5I,BTCOEX -  COEX_ANT_1 LinkOp=%u FreqOverlapping_true=%u AntFreq=%u AntBurstMode_True=%u LinkID=%u
35066,,BTCOEX -  COEX_ANT_2 
35067,,BTCOEX -  COEX_ENTER_NOA 
35068,,BTCOEX -  COEX_EXIT_NOA 
35069,,BTCOEX -  COEX_BT_SCAN_PROTECT 
35070,,BTCOEX -  COEX_DEBUG_ID_END 
35328,I,WLAN_MODULE_ROAM -  ROAM_DBGID_DEFINITION_START  0x%x
35329,,ROAM -  ROAM_MODULE_INIT 
35330,2I,ROAM_SCAN -  ROAM_VDEV_START vdev_id = %d roam_ctrl.running = %d
35331,2I,ROAM_SCAN -  ROAM_CONFIG_RSSI_THRESH  roam_scan_rssi_thresh = %d roam_rssi_thresh_diff = %d
35332,3I,ROAM_SCAN -  ROAM_CONFIG_SCAN_PERIOD  roam_scan_period = %d roam_scan_age = %d roam_ctrl.running = %d
35333,5I,ROAM_SCAN -  ROAM_CONFIG_AP_PROFILE  ssid_len = %d rssi_threshold = %d rsn_authmode = 0x%x rsn_mipher = 0x%x rsn_ucipher = 0x%x
35334,4I,ROAM_SCAN -  ROAM_CONFIG_CHAN_LIST  chan_list_type(FULL 0/CHANLIST 1/CHANMAP 2) = %d  num_chans = %d chan_list[0] = %d chan_list[1] = %d
35335,5I,ROAM_SCAN -  ROAM_CONFIG_SCAN_PARAMS_0 dwell_time_active = %d dwell_time_passive = %d burst_duration = %d min_rest_time = %d max_rest_time = %d
35336,2I,ROAM_SCAN -  ROAM_CONFIG_RSSI_CHANGE  val = %d bcn_rssi_weight = %d
35337,2I,ROAM_SCAN -  ROAM_SCAN_TIMER_START  roam_ctrl.running = %d roam_scan_mode(bitmap of PERIODIC 1/RSSI_CHANGE 2/BOTH 3/HO 4) = 0x%x
35338,2I,ROAM_SCAN -  ROAM_SCAN_TIMER_EXPIRE  roam_ctrl.running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d
35339,2I,ROAM_SCAN -  ROAM_SCAN_TIMER_STOP  roam_ctrl.running = %d roam_scan_mode(bitmap of PERIODIC 1/RSSI_CHANGE 2/BOTH 3/HO 4) = 0x%x
35340,3I,ROAM_SCAN -  ROAM_SCAN_STARTED    scan_id = 0x%x roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d bcn_rssi_avg = -%d dBm bcn_rssi_last = -%d dBm
35341,5I,ROAM_SCAN -  ROAM_SCAN_COMPLETE_0  candidate_found = 0x%x scan_info.scan_id = 0x%x roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d final_scan = %d send_bcn_to_host = %d
35342,4I,ROAM_SCAN -  ROAM_SCAN_CANCELLED  scan_id = 0x%x type = 0x%x reason = 0x%x scan_queue_status = 0x%x
35343,,ROAM_SCAN -  ROAM_CANDIDATE_FOUND 
35344,5I,ROAM_SCAN -  ROAM_RSSI_ACTIVE_SCAN  tmr_running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d start_scan = 0x%x prev_state = 0x%x final_scan = %d
35345,5I,ROAM_SCAN -  ROAM_RSSI_ACTIVE_ROAM  tmr_running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d start_scan = 0x%x prev_state = 0x%x final_scan = %d
35346,5I,ROAM_SCAN -  ROAM_RSSI_GOOD    bcn_rssi_avg = -%d dBm bcn_rssi_last = -%d dBm roam_scan_mode(PERIODIC 1/RSSI_CHANGE 2/BOTH 3/HO 4) = 0x%x prev_state = 0x%x tmr_running(bit1)/final_scan(bit0) = 0x%02x
35347,2I,ROAM_SCAN -  ROAM_BMISS_FIRST_RECV  roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d curr_rssi_avg = -%d dBm bcn_rssi_last = -%d dBm
35348,2I,ROAM_SCAN -  ROAM_VDEV_STOP  vdev_id = %d roam_ctrl.running = %d
35349,I,ROAM_SCAN -  ROAM_SCAN_OFFLOAD_ENABLE  enable = %d
35350,2I,ROAM_SCAN -  ROAM_CANDIDATE_SSID_MATCH  ieee_chan = %d scan_info.chan_freq = %d
35351,5I,ROAM_SCAN -  ROAM_CANDIDATE_SECURITY_MATCH  rsRssi = -%d dBm curr_rssi = -%d dBm scan_chan_map[ieee_chan/32] = 0x%x rssi_threshold = %d send_beacon_to_host = %d
35352,4I,ROAM_SCAN -  ROAM_LOW_RSSI_INTERRUPT  bcn_rssi_avg = -%d dBm bcn_rssi_last = -%d dBm hi_thresh = %d lo_thresh = %d
35353,4I,ROAM_SCAN -  ROAM_HIGH_RSSI_INTERRUPT  bcn_rssi_avg = -%d dBm bcn_rssi_last = -%d dBm hi_thresh = %d lo_thresh = %d
35354,5I,ROAM_SCAN -  ROAM_SCAN_REQUESTED_0  send_beacon_to_host = %d scan_type(FULL 0/CHANLIST 1/CHANMAP 2) = %d roam_scan_state (IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d final_scan = %d num_chan = %d
35355,3I,ROAM_SCAN -  ROAM_BETTER_CANDIDATE_FOUND  candidate_rssi_last = -%d dBm curr_rssi_avg = -%d dBm bcn_rssi_last = -%d dBm rssi_threshold = %d
35356,2I,ROAM_SCAN -  ROAM_BETTER_AP_EVENT  candidate_found = %d send_beacon_to_host = %d
35357,2I,ROAM_SCAN -  ROAM_CANCEL_LOW_PRIO_SCAN  send_beacon_to_host = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d 
35358,5I,ROAM_SCAN -  ROAM_FINAL_BMISS_RECVD  curr_rssi_avg = -%d dBm bcn_rssi_last = -%d dBm roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d scan_param.mode(bit3-1)/final_scan(bit0) = 0x%02x scan_status(bit2-1)/final_bmiss_recvd(bit0) = 0x%02x
35359,3I,ROAM_SCAN -  ROAM_CONFIG_SCAN_MODE  roam_scan_mode(PERIODIC 1/RSSI_CHANGE 2/BOTH 3/HO 4) = 0x%x roam_ctrl.running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d
35360,I,ROAM_SCAN -  ROAM_BMISS_FINAL_SCAN_ENABLE  enable = 0x%x
35361,2I,ROAM_SCAN -  ROAM_SUITABLE_AP_EVENT  candidate_found = %d send_beacon_to_host = %d
35362,3I,ROAM_SCAN -  ROAM_RSN_IE_PARSE_ERROR  rsn_ucipher = 0x%x rsn_mipher = 0x%x rsn_authmode = 0x%x 
35363,3I,ROAM_SCAN -  ROAM_WPA_IE_PARSE_ERROR  rsn_ucipher = 0x%x rsn_mipher = 0x%x rsn_authmode = 0x%x 
35364,3I,ROAM_SCAN -  ROAM_SCAN_CMD_FROM_HOST  command_arg = 0x%x  roam_ctrl.running = %d scan_status = %d
35365,3I,ROAM_HO -  ROAM_HO_SORT_CANDIDATE  total_candidate = %d best_urssi = %d sel_5g_margin = %d
35366,5I,ROAM_HO -  ROAM_HO_SAVE_CANDIDATE  idx = %d bssid = %08x:%04x rssi = -%d dBm prefer = %d 
35367,4I,ROAM_HO -  ROAM_HO_GET_CANDIDATE  blacklisted(bit31)_is_bcn(bit30)_total_cnd(hi_14)_cnd_idx(lo_16) = 0x%08x  bssid = %08x:%04x rssi = -%d dBm mhz = %d
35368,5I,ROAM_HO -  ROAM_HO_OFFLOAD_SET_PARAM  result(0/1/2/3) = %d flags/none/roam_scan_mode/rsn_authmode = 0x%x rssi_cat_gap = %d, sel_5g_margin = %d
35369,2I,ROAM_HO -  ROAM_HO_SM_ENTRY  entering state %d (INIT 0/WAIT_CH 1/PREAUTH 2/REASSOC 3/CONNECTED 4/AUTHENTICATED 5/SYNCH 6)
35370,5I,ROAM_HO -  ROAM_HO_HTT_CTRL_MSG intercept msg_type = 0x%x msg_bytes = 0x%x roam_vdev(hi)vdev(lo_16)/tid/sec_type = 0x%x (0xdead = not parsed) peer_id = 0x%x (0xdead = not parsed) => action = %d (save 1/drop 2/host 3)
35371,I,ROAM_HO -  ROAM_HO_SYNC_START prev_roam_state = %d
35372,,ROAM_HO -  ROAM_HO_START 
35373,I,ROAM_HO -  ROAM_HO_SYNC_COMPLETE error = 0x%x (HOST_ISSUE 0xfffffff)
35374,I,ROAM_HO -  ROAM_HO_STOP error_code = 0x%x (BMISS 1/HOST ISSUE 2/AUTH_SEND 3/AUTH_RECV 4/AUTH_TO 5/REASSOC_RECV 6/REASSOC_SEND 7/REASSOC_TO 8/EAP1X_RECV 9/DISCONNECT 10/EAPOL_TO 11/MLME 12) 
35375,2I,ROAM_HO -  ROAM_HO_HTT_FORWARD  forward_cnts = %d forward_bytes = %d
35376,5I,ROAM_SCAN - ROAM_CONFIG_SCAN_PARAMS_1 idle_time = %d max_scan_time = %d probe_delay = %d scan_ctrl_flags = 0x%x n_probes = %d
35377,2I,ROAM_SCAN - ROAM_SCAN_COMPLETE_1  reason(SUCC 0/CANCEL 1/PREEMPTED 2/TIMEOUT 3/INTERNAL FAIL 4) = %d evt_scan_id = 0x%x 
35378,4I,ROAM_SCAN - ROAM_SWBMISS_BCN_RECV_VAL bcn_rssi_last = -%d dBm evt->bcn_rssi_avg = -%d dBm change = %d rssi_change_val = %d
35379,3I,ROAM_SCAN -  ROAM_SWBMISS_BCN_RECV_THRE2 bcn_rssi_last = -%d dBm rssi_threshold2 = %d hit_rssi_thresh_cnt = %d
35380,1I,ROAM_SCAN -  ROAM_SCAN_REQUESTED_1 g_roam_req_scan_id = 0x%x
35381,2I,ROAM_HO -  ROAM_HO_SORT_CANDIDATE_CUR  cur_index = %d position = %d
35382,4I,ROAM_HO -  ROAM_HO_SAVE_CANDIDATE_DUP  duplicate candidate AP, bssid = %08x:%04x
35383,2I,ROAM_HO -  ROAM_HO_SM_EVENT  rcvd event = %d @ cur_state = %d (START_HO 0/CH_GRANT 1/PAUSED 2/MGMT_TX 3/MGMT_RX 4/SYNCH_COMP 5/SYNCH_FAIL 6/EV_CONNECT 7/EV_AUTH 8/EV_STOP_HO 9/EV_CH_END 10/EV_ERROR 11)
35384,5I,ROAM_HO -  ROAM_HO_ENTER_CH  roaming attempt to bssid = %08x:%04x (rssi = -%d dBm mhz = %d phy_mode = 0x%x)
35385,2I,ROAM_HO -  ROAM_HO_MGMT_RX subtype = %d status_code = %d
35386,5I,ROAM_HO -  ROAM_HO_CANDIDATE_INFO  mhz = %d phy_mode = %d cap = %d is_erp = %d has_11b_rate = %d
35387,5I,ROAM_HO -  ROAM_HO_OFFLD_DATA_STORE store incoming data vdev_id = 0x%x peer_id = 0x%x tid = 0x%x pkt_len = %d -> ret_val = 0x%x
35388,5I,ROAM_HO -  ROAM_HO_HTT_DATA intercept msg_type = 0x%x msg_bytes = 0x%x peer_id = 0x%x count = %d  remaining_size = %d
35389,2I,ROAM_HO -  ROAM_HO_UPDATE_STATUS  rcvd status = %d @ cur_state = %d (SUCC 0/4WAY_FINISHED 1/EAP1X 2/SYNC_START 3/SYNC_DONE 4/ABORT 5/DISCONNECT 6)
35390,2I,ROAM_HO -  ROAM_HO_OCS_CH_CB  rcvd event = %d @ cur_state = %d (GRANTED 0/COMPLETED 1/STOPPED 2/PREEMPTED 3/END 4)
35391,3I,ROAM_HO -  ROAM_RSSI_INTERRUPT_STATE  Roam Intr State SubID = %d  Par1  = %d Par2  = %d
35392,5I,ROAM_SCAN - ROAM_INVOKE_PARAM_CHECK invoke_roam_scan_mode = %d ap_sel_mode = %d roam_delay = %d num_chan = %d num_bssid = %d
35393,1I,ROAM_SCAN - ROAM_INVOKE_PARAM_CHAN channel = %d
35394,2I,ROAM_SCAN - ROAM_INVOKE_PARAM_BSSID BSSID low = 0x%08x high = 0x%08x
35395,4I,ROAM_SCAN - ROAM_INVOKE_STATE_CHECK roam_offload = %d in_use = %d scan_mode = %d ap ssid_len = %d
35396,1I,ROAM_SCAN - ROAM_INVOKE_START_SUCCESS roam_scan_type = %d
35397,1I,ROAM_SCAN - ROAM_INVOKE_START_FAILURE error code = 0x%x
35398,3I,ROAM_SCAN - ROAM_INVOKE_BSSID_CHECK Recv BSSID low = 0x%08x high = 0x%08x DROP = %d
35399,,WLAN_MODULE_ROAM -  ROAM_DBGID_DEFINITION_END 
35828,I, ROAM_SM - ROAM_SM [transition 0/dispatch 1/warning 2]/[old state/current state/error type]/[new state/event id/rsvd]/[rsvd] = 0x%08x
35840,,WLAN_MODULE_RESMGR_CHAN_MANAGER - RESMGR_CHMGR_DEFINITION_START 
35841,3I,CHAN_MANAGER - Pause Completed. Pause Status/Link = 0x%x, Curr Wal Time/Link Flags/Cur VC = 0x%x,Ch Mgr State/NA = 0x%x
35842,I,CHAN_MANAGER - Channel Change - 0x%x mhz
35843,,CHAN_MANAGER - Resume Complete 
35844,4I,CHAN_MANAGER - Pause VDEV at channel 0x%x mhz. Link = 0x%x Pause Time =  0x%x us Curr WAL Time = 0x%x us
35845,3I,CHAN_MANAGER - UnPause VDEV at channel 0x%x. Link = 0x%x Curr WAL Time = 0x%x us
35846,2I,CHAN_MANAGER - CTS2S TX Failed. Status = 0x%x OCS CTX = 0x%x
35847,2I,CHAN_MANAGER - CFEND TX Failed. Status = 0x%x OCS CTX = 0x%x
35848,,WLAN_MODULE_RESMGR_CHAN_MANAGER - RESMGR_CHMGR_DEFINITION_END 
36352,,WLAN_MODULE_RESMGR -  RESMGR_DEFINITION_START 
36353,I,RESMGR -  RESMGR_OCS_ALLOCRAM_SIZE  size_in_bytes = %d
36354,5I,RESMGR -  RESMGR_OCS_RESOURCES  req_id/num_vdev/arg1 = 0x%x ch_req_addr/ch_alloc_entries/arg2 = 0x%x ch_alloc_addr = 0x%x state = 0x%x priority_chanmhz = 0x%x
36355,I,RESMGR -  RESMGR_LINK_CREATE  link_address = 0x%x
36356,I,RESMGR -  RESMGR_LINK_DELETE  link_address = 0x%x
36357,5I,RESMGR -  RESMGR_OCS_CHREQ_CREATE  start_tsf/req_id = 0x%x duration_usec/dtim_start_tsf = 0x%x interval/dtim_period=%d prioirty_chanmhz/purge_flag = 0x%x chan_req_addr/end_tsf = 0x%x
36358,5I,RESMGR -  RESMGR_OCS_CHREQ_DELETE  req_id = 0x%x chan_req_addr = 0x%x chann_alloc_addr = 0x%x state = %d priority_chanmhz = 0x%x
36359,5I,RESMGR -  RESMGR_OCS_CHREQ_START  start_tsf/req_id = 0x%x duration_usec/dtim_start_tsf = 0x%x interval/dtim_period=%d prioirty_chanmhz/purge_flag = 0x%x chan_req_addr/end_tsf = 0x%x
36360,5I,RESMGR -  RESMGR_OCS_CHREQ_STOP  req_id = 0x%x chan_req_addr = 0x%x chann_alloc_addr = 0x%x state = %d priority_chanmhz = 0x%x
36361,2I,RESMGR -  RESMGR_OCS_SCHEDULER_INVOKED  current_tsf/curr_ch_alloc_addr = 0x%x current_time = 0x%x
36362,2I,RESMGR -  RESMGR_OCS_CHREQ_GRANT  curr_time = 0x%x ch_req_addr = 0x%x
36363,2I,RESMGR -  RESMGR_OCS_CHREQ_COMPLETE  curr_time = 0x%x ch_req_addr = 0x%x
36364,I,RESMGR -  RESMGR_OCS_NEXT_TSFTIME  next_tsf_time = 0x%x
36365,I,RESMGR -  RESMGR_OCS_TSF_TIMEOUT_US  timeout_us = %d
36366,,RESMGR -  RESMGR_OCS_CURR_CAT_WINDOW 
36367,3I,RESMGR -  RESMGR_OCS_CURR_CAT_WINDOW_REQ  req_id = 0x%x ch_req_addr = 0x%x state = %d
36368,2I,RESMGR -  RESMGR_OCS_CURR_CAT_WINDOW_TIMESLOT  start_tsf = 0x%x stop_tsf = 0x%x
36369,4I,RESMGR -  RESMGR_OCS_CHREQ_RESTART  start_tsf = 0x%x stop_tsf = 0x%x dtim_start_tsf = 0x%x dtim_period = %d
36370,I,RESMGR -  RESMGR_OCS_CLEANUP_CH_ALLOCATORS  cur_ch_alloc_addr = 0x%x
36371,2I,RESMGR -  RESMGR_OCS_PURGE_CHREQ  cur_ch_alloc_addr/cur_ch_req_addr = 0x%x chan_mhz = 0x%x
36372,I,RESMGR -  RESMGR_OCS_CH_ALLOCATOR_FREE  cur_ch_alloc_addr = 0x%x
36373,,RESMGR -  RESMGR_OCS_RECOMPUTE_SCHEDULE 
36374,2I,RESMGR -  RESMGR_OCS_NEW_CAT_WINDOW_REQ  ch_req_addr = 0x%x state = %d
36375,2I,RESMGR -  RESMGR_OCS_NEW_CAT_WINDOW_TIMESLOT  start_tsf = 0x%x stop_tsf = 0x%x
36376,2I,RESMGR -  RESMGR_OCS_CUR_CH_ALLOC  curr_chan_alloc_addr = 0x%x chan_mhz = 0x%x
36377,2I,RESMGR -  RESMGR_OCS_WIN_CH_ALLOC  winning_chan_alloc_addr = 0x%x chan_mhz = 0x%x
36378,,RESMGR -  RESMGR_OCS_SCHED_CH_CHANGE 
36379,2I,RESMGR -  RESMGR_OCS_CONSTRUCT_CAT_WIN  chan_alloc_addr = 0x%x chan_mhz=0x%x
36380,2I,RESMGR -  RESMGR_OCS_CHREQ_PREEMPTED  curr_time = 0x%x ch_req_addr = 0x%x
36381,,RESMGR -  RESMGR_OCS_CH_SWITCH_REQ 
36382,I,RESMGR -  RESMGR_OCS_CHANNEL_SWITCHED  status = %d
36383,I,RESMGR -  RESMGR_OCS_CLEANUP_STALE_REQS  cur_ch_alloc_addr = 0x%x
36384,5I,RESMGR -  RESMGR_OCS_CHREQ_UPDATE  start_tsf/req_id = 0x%x duration_usec/dtim_start_tsf = 0x%x interval/dtim_period=%d prioirty_chanmhz/purge_flag = 0x%x chan_req_addr/end_tsf = 0x%x
36385,,RESMGR -  RESMGR_OCS_REG_NOA_NOTIF 
36386,,RESMGR -  RESMGR_OCS_DEREG_NOA_NOTIF 
36387,,RESMGR -  RESMGR_OCS_GEN_PERIODIC_NOA
36388,2I,RESMGR -  RESMGR_OCS_RECAL_QUOTAS  num_home_chans/chan_mhz = %d tracking_interval/latency = %d
36389,2I,RESMGR -  RESMGR_OCS_GRANTED_QUOTA_STATS  chan_mhz = %d chan_time_granted_us = %d
36390,3I,RESMGR -  RESMGR_OCS_ALLOCATED_QUOTA_STATS  chan_mhz = %d req_chan_time_percentage = %d chan_time_quota = %d
36391,3I,RESMGR -  RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x chan_mhz = 0x%x req_chan_time/latency = 0x%x
36392,I,RESMGR -  RESMGR_OCS_TRACKING_TIME_FIRED  curr_chan_alloc_addr = 0x%x
36393,5I,RESMGR -  RESMGR_VC_ARBITRATE_ATTRIBUTES  chan_mhz = %d phy_mode/vc_prog_latency = %d band_center_freq = %d virtual_chan_ctxt = 0x%x virtual_chan = 0x%x
36394,2I,RESMGR -  RESMGR_OCS_LATENCY_STRICT_TIME_SLOT  slot1_start_tsf = 0x%x slot2_start_tsf = 0x%x
36395,I,RESMGR -  RESMGR_OCS_CURR_TSF  current_tsf = 0x%x
36396,2I,RESMGR -  RESMGR_OCS_QUOTA_REM  cat1_quota_remain = 0x%x cat2_quota_remain = 0x%x
36397,I,RESMGR -  RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x
36398,I,RESMGR -  RESMGR_OCS_WIN_CAT_DUR  duration = 0x%x
36399,I,RESMGR -  RESMGR_VC_UPDATE_CUR_VC  chan_mhz = %d
36400,4I,RESMGR -  RESMGR_VC_REG_UNREG_LINK  reg_unreg/arg1 = 0x%x chan_mhz/arg2 = 0x%x home_chan_count/link_count/arg3 = 0x%x virtual_chan_count/ephemeral_link_count/arg4 = 0x%x
36401,2I,RESMGR -  RESMGR_VC_PRINT_LINK  link_flags = 0x%x link_valid_attr = 0x%x
36402,2I,RESMGR -  RESMGR_OCS_MISS_TOLERANCE  miss_tolerance_cnt_timeslot1 = 0x%x miss_tolerance_cnt_timeslot2 = 0x%x
36403,I,RESMGR -  RESMGR_DYN_SCH_ALLOCRAM_SIZE  size = %d
36404,2I,RESMGR -  RESMGR_DYN_SCH_ENABLE  enable = 0x%x fw_disable_bmap = 0x%x
36405,I,RESMGR -  RESMGR_DYN_SCH_ACTIVE  is_active = %d
36406,5I,RESMGR -  RESMGR_DYN_SCH_CH_STATS_START  chan_mhz = %d start_rx_clear_cnt = %d start_tx_frame_cnt = %d start_rx_frame_cnt_us = %d start_time_us = %d
36407,4I,RESMGR -  RESMGR_DYN_SCH_CH_SX_STATS  chan_mhz = %d accu_tx_rx_dur_us = 0x%x accu_free_dur_us = 0x%x accu_sampling_dur_us = 0x%x
36408,2I,RESMGR -  RESMGR_DYN_SCH_TOT_UTIL_PER  chan_mhz = %d chan_util_percentage = %d
36409,2I,RESMGR -  RESMGR_DYN_SCH_HOME_CH_QUOTA  chan_mhz = %d ch_new_quota = %d
36410,2I,RESMGR -  RESMGR_OCS_REG_RECAL_QUOTA_NOTIF  handler/arg1 = 0x%x arg2 = 0x%x
36411,2I,RESMGR -  RESMGR_OCS_DEREG_RECAL_QUOTA_NOTIF  handler/arg1 = 0x%x arg2 = 0x%x
36412,5I,RESMGR -  RESMGR_DYN_SCH_CH_STATS_END  chan_mhz = %d rx_clear_cnt = %d tx_frame_cnt = %d rx_frame_cnt_us = %d sampling_dur_us = %d
36413,,WLAN_MODULE_RESMGR -  RESMGR_DEFINITION_END
36864,,WLAN_MODULE_VDEV_MGR -  VDEV_MGR_DEFINITION_START 
36865,I,VDEV_MGR -  VDEV_MGR_FIRST_BMISS_DETECTED  vdev_id/info = 0x%x
36866,I,VDEV_MGR -  VDEV_MGR_FINAL_BMISS_DETECTED  vdev_id = 0x%x
36867,3I,VDEV_MGR -  VDEV_MGR_BCN_IN_SYNC  vdev_id/arg1 = 0x%x curr_tsf/arg2 = 0x%x wal_vdev_tsf/arg3 = 0x%x
36868,3I,VDEV_MGR -  VDEV_MGR_AP_KEEPALIVE_IDLE  assoc_id = 0x%x inact_gen = 0x%x n_buffered_mpdu = 0x%x
36869,4I,VDEV_MGR -  VDEV_MGR_AP_KEEPALIVE_INACTIVE  assoc_id/now = 0x%x inact_gen/last_txrx_time = 0x%x n_buffered_mpdu/last_tx_time = 0x%x last_rx_time = 0x%x
36870,3I,VDEV_MGR -  VDEV_MGR_AP_KEEPALIVE_UNRESPONSIVE  assoc_id = 0x%x inact_gen = 0x%x n_buffered_mpdu = 0x%x
36871,4I,VDEV_MGR -  VDEV_MGR_AP_TBTT_CONFIG  chan_mhz = %d link_type = 0x%x interval = 0x%x offset = 0x%x
36872,3I,VDEV_MGR -  VDEV_MGR_FIRST_BCN_RECEIVED  curr_time/vdev_id = 0x%x seq = 0x%x rssi = 0x%x
36873,4I,VDEV_MGR -  VDEV_MGR_VDEV_START  vdev_id = 0x%x chan_mhz = %d mode = 0x%x sub_mode = 0x%x
36874,I,VDEV_MGR -  VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x
36875,I,VDEV_MGR -  VDEV_MGR_PEER_AUTHORIZED  vdev_id = 0x%x
36876,3I,VDEV_MGR -  VDEV_MGR_OCS_HP_LP_REQ_POSTED  vdev_id = 0x%x hp_req = 0x%x lp_req = 0x%x
36877,2I,VDEV_MGR -  VDEV_MGR_VDEV_START_OCS_HP_REQ_COMPLETE  vdev_id = 0x%x ch_req_flag = 0x%x
36878,I,VDEV_MGR -  VDEV_MGR_VDEV_START_OCS_HP_REQ_STOP  vdev_id = 0x%x
36879,4I,VDEV_MGR -  VDEV_MGR_HP_START_TIME  vdev_id = 0x%x chan_mhz = %d start_tsf = 0x%x duration = 0x%x
36880,5I,VDEV_MGR -  VDEV_MGR_VDEV_PAUSE_DELAY_UPDATE  arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x arg5 = 0x%x
36881,I,VDEV_MGR -  VDEV_MGR_VDEV_PAUSE_FAIL  arg = 0x%x
36882,,VDEV_MGR -  VDEV_MGR_GEN_PERIODIC_NOA 
36883,4I,VDEV_MGR -  VDEV_MGR_OFF_CHAN_GO_CH_REQ_SETUP  arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x
36884,,WLAN_MODULE_VDEV_MGR -  VDEV_MGR_DEFINITION_END 
37376,I,WLAN_MODULE_SCAN -  SCAN_START_COMMAND_FAILED  0x%x
37377,I,WLAN_MODULE_SCAN -  SCAN_STOP_COMMAND_FAILED  0x%x
37378,I,WLAN_MODULE_SCAN -  SCAN_EVENT_SEND_FAILED  0x%x
37379,5I,WLAN_MODULE_SCAN -  SCAN_ENGINE_START  0x%x 0x%x 0x%x 0x%x 0x%x
37380,2I,WLAN_MODULE_SCAN -  SCAN_ENGINE_CANCEL_COMMAND  0x%x 0x%x
37381,5I,WLAN_MODULE_SCAN -  SCAN_ENGINE_STOP_DUE_TO_TIMEOUT  0x%x 0x%x 0x%x 0x%x 0x%x
37382,2I,WLAN_MODULE_SCAN -  SCAN_EVENT_SEND_TO_HOST  0x%x 0x%x
37383,5I,WLAN_MODULE_SCAN -  SCAN_EVENT_ADD  0x%x 0x%x 0x%x 0x%x 0x%x
37384,4I,WLAN_MODULE_SCAN -  SCAN_EVENT_REM  0x%x 0x%x 0x%x 0x%x
37385,3I,WLAN_MODULE_SCAN -  SCAN_EVENT_PREEMPTED  0x%x 0x%x 0x%x
37386,I,WLAN_MODULE_SCAN -  SCAN_EVENT_RESTARTED  0x%x
37387,2I,WLAN_MODULE_SCAN -  SCAN_EVENT_COMPLETED  0x%x 0x%x
37388,,WLAN_MODULE_SCAN -  SCAN_SM_REQ_NEXT_CH 
37389,,WLAN_MODULE_SCAN -  SCAN_DBGID_DEFINITION_END 
37888,,WLAN_MODULE_RATECTRL -  RATECTRL_DBGID_DEFINITION_START 
37889,5I,RATECTRL -  RATECTRL_DBGID_ASSOC  TxChainMask=0x%x PhyMode=0x%x Flags=0x%x VhtSet=0x%x HtSet=0x%x
37890,I,RATECTRL -  RATECTRL_DBGID_NSS_CHANGE  Nss=0x%x
37891,,RATECTRL -  RATECTRL_DBGID_CHAINMASK_ERR 
37892,,RATECTRL -  RATECTRL_DBGID_UNEXPECTED_FRAME 
37893,5I,RATECTRL -  RATECTRL_DBGID_WAL_RCQUERY  rix0=0x%x rix1=0x%x rix2=0x%x ProbeRix=0x%x SwPpduFlags=0x%x
37894,2I,RATECTRL -  RATECTRL_DBGID_WAL_RCUPDATE  NumTxDnElem=0x%x SwPpduFlags=0x%x
37895,6I,RATECTRL -  RATECTRL_DBGID_GTX_UPDATE  0x%x 0x%x 0x%x 0x%x 0x%x 0x%x
37896,,WLAN_MODULE_RATECTRL -  RATECTRL_DBGID_DEFINITION_END 
38400,,WLAN_MODULE_AP_PWRSAVE -  AP_PS_DBGID_DEFINITION_START 
38401,2I,AP_PWRSAVE -  AP_PS_DBGID_UPDATE_TIM AssocID = %d IsTimSet = %d
38402,3I,AP_PWRSAVE -  AP_PS_DBGID_PEER_STATE_CHANGE PeerType = %d AssocID = %d PwrMgmt = %d
38403,3I,AP_PWRSAVE -  AP_PS_DBGID_PSPOLL AssocID = %d Tid = %d Flags = 0x%x
38404,I,AP_PWRSAVE -  AP_PS_DBGID_PEER_CREATE AssocID = %d
38405,I,AP_PWRSAVE -  AP_PS_DBGID_PEER_DELETE AssocID = %d
38406,,AP_PWRSAVE -  AP_PS_DBGID_VDEV_CREATE 
38407,,AP_PWRSAVE -  AP_PS_DBGID_VDEV_DELETE 
38408,3I,AP_PWRSAVE -  AP_PS_DBGID_SYNC_TIM AssocID = %d Tids = 0x%x TimSet = %d
38409,4I,AP_PWRSAVE -  AP_PS_DBGID_NEXT_RESPONSE AssocID = %d USPActive = %d PendingUSP = %d PendingPollResp = %d
38410,3I,AP_PWRSAVE -  AP_PS_DBGID_START_SP AssocID = %d Timestamp = %d Mark = %d
38411,3I,AP_PWRSAVE -  AP_PS_DBGID_COMPLETED_EOSP AssocID = %d Timestamp = %d LastRxTriggerTime = %d
38412,4I,AP_PWRSAVE -  AP_PS_DBGID_TRIGGER AssocID = %d Timestamp = %d USPActive = %d SendNInProgress = %d
38413,4I,AP_PWRSAVE -  AP_PS_DBGID_DUPLICATE_TRIGGER AssocID = %d Timestamp = %d SeqNO = %d Tid = %d
38414,5I,AP_PWRSAVE -  AP_PS_DBGID_UAPSD_RESPONSE AssocID = %d Tid = %d NumMPDUToSend = %d Flags = %d SPLength = 0x%x
38415,5I,AP_PWRSAVE -  AP_PS_DBGID_SEND_COMPLETE AssocID = %d FrameCtrl = 0x%x QoSCtrl = 0x%x USPActive = %d PendingPollResp = %d
38416,3I,AP_PWRSAVE -  AP_PS_DBGID_SEND_N_COMPLETE AssocID = %d USPActive = %d PendingPollResp = %d
38417,4I,AP_PWRSAVE -  AP_PS_DBGID_DETECT_OUT_OF_SYNC_STA AssocID = %d Timestamp = %d OldestTxBufferedWaitingMs = %d QDepeth = %d
38418,4I,AP_PWRSAVE -  AP_PS_DBGID_DELIVER_CAB Tid = %d NumMPDU = %d Flags = 0x%x RetryOther = %d
38419,4I,AP_PWRSAVE -  AP_PS_DBGID_PSPOLL_REQ AssocID = %d Aid = %d PeerPSEnabled = %d SendNInProgress = %d
38420,4I,AP_PWRSAVE -  AP_PS_DBGID_PSPOLL_ERROR AssocID = %d TidPaused = %d AllowdLegacyTidMask = 0x%x LegacyTidMask = 0x%x
38421,5I,AP_PWRSAVE -  AP_PS_DBGID_UAPSD_RESPONSE_ERROR AssocID = %d Tid/Paused = 0x%x AllowedUAPSDTidMask = 0x%x PendingTidMap = 0x%x SPLength = 0x%x
38422,3I,AP_PWRSAVE -  AP_PS_DBGIG_SET_PARAM AssocID = %d Param = %d Value = %d
38423,3I,AP_PWRSAVE -  AP_PS_DBGIG_UAPSD_CFG AssocID = %d UAPSDTriggerTids = 0x%x UAPSDDeliveryTids = 0x%x
38424,,AP_PWRSAVE -  AP_PS_DBGID_PS_DESC_BIN_HWM Bitmap = 0x%x VdevMap = 0x%x
38425,,AP_PWRSAVE -  AP_PS_DBGID_PS_DESC_BIN_LWM Bitmap = 0x%x VdevMap = 0x%x
38426,2I,AP_PWRSAVE -  AP_PS_DBGID_HOST_TX_PAUSE 0x%x 0x%x
38427,,AP_PWRSAVE -  AP_PS_DBGID_NO_CLIENT 
38428,,AP_PWRSAVE -  AP_PS_DBGID_CLIENT_IN_PS_ACTIVE 
38429,,AP_PWRSAVE -  AP_PS_DBGID_CLIENT_IN_PS_NON_ACTIVE 
38430,,AP_PWRSAVE -  AP_PS_DBGID_CLIENT_IN_AWAKE
38912,,WLAN_MODULE_BLOCKACK
39424,,WLAN_MODULE_MGMT_TXRX -  MGMT_TXRX_DBGID_DEFINITION_START 
39425,3I,MGMT_TXRX -  MGMT_TXRX_FORWARD_TO_HOST  Channel_VdevActiveCount_Channel=0x%x Seq_Type_Subtype=0x%x 0x%x
39426,,WLAN_MODULE_MGMT_TXRX -  MGMT_TXRX_DBGID_DEFINITION_END 
39936,,WLAN_MODULE_DATA_TXRX -  DATA_TXRX_DBGID_DEFINITION_START
39937,3I,DATA_TXRX - DATA_TXRX_DBGID_RX_DATA_SEQ_LEN_INFO Invalid Peer 0x%x 0x%x Err=0x%x
39938,4I,DATA_TXRX -  DATA_TXRX_DBGID_REPLAY_CHECK 0x%x KeyId=0x%x oldPN=0x%x newPN=0x%x
39939,5I,DATA_TXRX -  DATA_TXRX_DBGID_DUP_CHECK SN=0x%x Len=0x%x Err=0x%x WalRxCnt=0x%x DataRxCnt=0x%x
39942,,DATA_TXRX -  DATA_TXRX_INVALID_ADDR1_STA Invalid Addr1 frame recd
39943,,DATA_TXRX -  DATA_TXRX_INVALID_ADDR1_P2P Invalid Addr1 frame recd
39944,,WLAN_MODULE_DATA_TXRX -  DATA_TXRX_DBGID_DEFINITION_END
40448,,WLAN_MODULE_HTT - HTT_DBGID_DEFINITION_START
40449,I,HTT - HTT_DBGID_INVALID_VDEVID_OR_GROUP desc0=x%x
40450,3I,HTT - HTT_DBGID_DISCARD_INTERNAL_PKTS vdev_mask=x%x quota=x%x frames=x%x
40451,5I,HTT - HTT_DBGID_DISCARD_TX_PKTS G=x%x frames=x%x quota=x%x desc0=x%x desc1=x%x
40452,3I,HTT - HTT_DBGID_GROUP_CHANGE vdev_id=x%x mhz=%d join=x%x 
40453,6I,HTT - HTT_DBGID_GROUP_CREDIT_STATS G=x%x vdev_mask=x%x quota=x%x pending=x%x frames=x%x reap=x%x
40454,2I,HTT - HTT_DBGID_DISCARD_INTERNAL_PKTS_NUM vdev_mask=x%x dropped=%d
40455,,WLAN_MODULE_HTT - HTT_DBGID_DEFINITION_END
40960,,WLAN_MODULE_HOST
41472,,BEACON -  BEACON_EVENT_SWBA_SEND_FAILED 
41473,3I,BEACON -  EARLY_RX_BMISS_STATUS  rcv %d total %d miss %d
41474,I,BEACON -  BEACON_EVENT_EARLY_RX_SLEEP_SLOP  %d
41475,I,BEACON -  BEACON_EVENT_EARLY_RX_CONT_BMISS_TIMEOUT  sleep_slop %d
41476,I,BEACON -  BEACON_EVENT_EARLY_RX_PAUSE_SKIP_BCN_NUM  %d
41477,I,BEACON -  BEACON_EVENT_EARLY_RX_CLK_DRIFT  %d
41478,I,BEACON -  BEACON_EVENT_EARLY_RX_AP_DRIFT  %d
41479,I,BEACON -  BEACON_EVENT_EARLY_RX_BCN_TYPE  %d
41480,2I,BEACON -  BEACON_EVENT_TSFOOR 0x%x 0x%x
41984,,WLAN_MODULE_OFFLOAD -  OFFLOAD_MGR_DBGID_DEFINITION_START 
41985,2I,OFFLOAD -  OFFLOADMGR_REGISTER_OFFLOAD  offload_module = 0x%x ref_cnt = 0x%x
41986,2I,OFFLOAD -  OFFLOADMGR_DEREGISTER_OFFLOAD  offload_module = 0x%x ref_cnt = 0x%x
41987,2I,OFFLOAD -  OFFLOADMGR_NO_REG_DATA_HANDLERS CE_send_entries_avail = 0x%x CE_recv_entries_avail = 0x%x
41988,,OFFLOAD -  OFFLOADMGR_NO_REG_EVENT_HANDLERS
41989,,OFFLOAD -  OFFLOADMGR_REG_OFFLOAD_FAILED 
41990,I,OFFLOAD -  OFFLOADMGR_DEREG_OFFLOAD_FAILED  offload_module = 0x%x
41991,I,OFFLOAD -  OFFLOADMGR_ENTER_FAILED  offload_module = 0x%x
41992,2I,OFFLOAD -  OFFLOADMGR_EXIT_FAILED  offload_module = 0x%x extra_id = 0x%x
41993,,WLAN_MODULE_OFFLOAD -  OFFLOADMGR_DBGID_DEFINITION_END 
42496,,WLAN_MODULE_WAL -  WAL_DBGID_DEFINITION_START 
42497,,WLAN_MODULE_WAL -  WAL_DBGID_FAST_WAKE_REQUEST 
42498,,WLAN_MODULE_WAL -  WAL_DBGID_FAST_WAKE_RELEASE 
42499,3I,WAL -  WAL_DBGID_SET_POWER_STATE  current = 0x%x desired = 0x%x fast_wake_req_count = %d
42500,,WLAN_MODULE_WAL -  WAL_DBGID_4
42501,4I,WLAN_MODULE_WAL -  WAL_DBGID_CHANNEL_CHANGE_FORCE_RESET  0x%x 0x%x 0x%x 0x%x
42502,2I,WLAN_MODULE_WAL -  WAL_DBGID_CHANNEL_CHANGE  0x%x 0x%x
42503,2I,WLAN_MODULE_WAL -  WAL_DBGID_VDEV_START  0x%x 0x%x
42504,I,WLAN_MODULE_WAL -  WAL_DBGID_VDEV_STOP  0x%x
42505,2I,WLAN_MODULE_WAL -  WAL_DBGID_VDEV_UP  0x%x 0x%x
42506,2I,WLAN_MODULE_WAL -  WAL_DBGID_VDEV_DOWN  0x%x 0x%x
42507,5I,WLAN_MODULE_WAL -  WAL_DBGID_SW_WDOG_RESET  0x%x 0x%x 0x%x 0x%x 0x%x
42508,5I,WLAN_MODULE_WAL -  WAL_DBGID_TX_SCH_REGISTER_TIDQ  0x%x 0x%x 0x%x 0x%x 0x%x
42509,5I,WLAN_MODULE_WAL -  WAL_DBGID_TX_SCH_UNREGISTER_TIDQ  0x%x 0x%x 0x%x 0x%x 0x%x
42510,5I,WLAN_MODULE_WAL -  WAL_DBGID_TX_SCH_TICKLE_TIDQ  0x%x 0x%x 0x%x 0x%x 0x%x
42511,2I,WLAN_MODULE_WAL -  WAL_DBGID_XCESS_FAILURES  0x%x 0x%x
42512,5I,WLAN_MODULE_WAL -  WAL_DBGID_AST_ADD_WDS_ENTRY  0x%x 0x%x 0x%x 0x%x 0x%x
42513,3I,WLAN_MODULE_WAL -  WAL_DBGID_AST_DEL_WDS_ENTRY  0x%x 0x%x 0x%x
42514,4I,WLAN_MODULE_WAL -  WAL_DBGID_AST_WDS_ENTRY_PEER_CHG  0x%x 0x%x 0x%x 0x%x
42515,2I,WLAN_MODULE_WAL -  WAL_DBGID_AST_WDS_SRC_LEARN_FAIL  0x%x 0x%x
42516,I,WLAN_MODULE_WAL -  WAL_DBGID_STA_KICKOUT  0x%x
42517,4I,WLAN_MODULE_WAL -  WAL_DBGID_BAR_TX_FAIL  assoc_id=0x%x tid_num=0x%x tid_qdepth=0x%x seq_num=%d
42518,,WLAN_MODULE_WAL -  WAL_DBGID_BAR_ALLOC_FAIL 
42519,,WLAN_MODULE_WAL -  WAL_DBGID_LOCAL_DATA_TX_FAIL 
42520,,WLAN_MODULE_WAL -  WAL_DBGID_SECURITY_PM4_QUEUED 
42521,,WLAN_MODULE_WAL -  WAL_DBGID_SECURITY_GM1_QUEUED 
42522,,WLAN_MODULE_WAL -  WAL_DBGID_SECURITY_PM4_SENT 
42523,I,WLAN_MODULE_WAL -  WAL_DBGID_SECURITY_ALLOW_DATA  0x%x
42524,I,WLAN_MODULE_WAL -  WAL_DBGID_SECURITY_UCAST_KEY_SET  0x%x
42525,I,WLAN_MODULE_WAL -  WAL_DBGID_SECURITY_MCAST_KEY_SET  0x%x
42526,,WLAN_MODULE_WAL -  WAL_DBGID_SECURITY_ENCR_EN 
42527,4I,WLAN_MODULE_WAL -  WAL_DBGID_BB_WDOG_TRIGGERED  0x%x 0x%x 0x%x 0x%x
42528,I,WLAN_MODULE_WAL -  WAL_DBGID_RX_LOCAL_BUFS_LWM  0x%x
42529,I,WLAN_MODULE_WAL -  WAL_DBGID_RX_LOCAL_DROP_LARGE_MGMT  0x%x
42530,I,WLAN_MODULE_WAL -  WAL_DBGID_VHT_ILLEGAL_RATE_PHY_ERR_DETECTED  0x%x
42531,3I,WLAN_MODULE_WAL -  WAL_DBGID_DEV_RESET  0x%x 0x%x 0x%x
42532,5I,WLAN_MODULE_WAL -  WAL_DBGID_TX_BA_SETUP  0x%x 0x%x 0x%x 0x%x 0x%x
42533,5I,WLAN_MODULE_WAL -  WAL_DBGID_RX_BA_SETUP  0x%x 0x%x 0x%x 0x%x 0x%x
42534,5I,WLAN_MODULE_WAL -  WAL_DBGID_DEV_TX_TIMEOUT  0x%x 0x%x 0x%x 0x%x 0x%x
42535,,WLAN_MODULE_WAL -  WAL_DBGID_DEV_RX_TIMEOUT 
42536,I,WLAN_MODULE_WAL -  WAL_DBGID_STA_VDEV_XRETRY  0x%x
42537,,WLAN_MODULE_WAL -  WAL_DBGID_DCS 
42538,2I,WLAN_MODULE_WAL -  WAL_DBGID_MGMT_TX_FAIL  0x%x 0x%x
42539,I,WLAN_MODULE_WAL -  WAL_DBGID_SET_M4_SENT_MANUALLY  0x%x
42540,I,WLAN_MODULE_WAL -  WAL_DBGID_PROCESS_4_WAY_HANDSHAKE  0x%x
42541,2I,WLAN_MODULE_WAL -  WAL_DBGID_WAL_CHANNEL_CHANGE_START  0x%x 0x%x
42542,5I,WLAN_MODULE_WAL -  WAL_DBGID_WAL_CHANNEL_CHANGE_COMPLETE  0x%x 0x%x 0x%x 0x%x 0x%x
42543,2I,WLAN_MODULE_WAL -  WAL_DBGID_WHAL_CHANNEL_CHANGE_START  0x%x 0x%x
42544,2I,WLAN_MODULE_WAL -  WAL_DBGID_WHAL_CHANNEL_CHANGE_COMPLETE  0x%x 0x%x
42545,4I,WLAN_MODULE_WAL -  WAL_DBGID_TX_MGMT_DESCID_SEQ_TYPE_LEN  0x%x 0x%x 0x%x 0x%x
42546,4I,WLAN_MODULE_WAL -  WAL_DBGID_TX_DATA_MSDUID_SEQ_TYPE_LEN tid_num=0x%x 0x%x 0x%x num_mpdus=0x%x
42547,I,WLAN_MODULE_WAL -  WAL_DBGID_TX_DISCARD  0x%x
42548,3I,WLAN_MODULE_WAL -  WAL_DBGID_TX_MGMT_COMP_DESCID_STATUS  0x%x 0x%x 0x%x
42549,3I,WLAN_MODULE_WAL -  WAL_DBGID_TX_DATA_COMP_MSDUID_STATUS  tid_and_msdu_num=0x%x tx_comp_status=0x%x ppdu_ssn=0x%x 
42550,I,WLAN_MODULE_WAL -  WAL_DBGID_RESET_PCU_CYCLE_CNT  0x%x
42551,3I,WLAN_MODULE_WAL -  WAL_DBGID_SETUP_RSSI_INTERRUPTS  0x%x 0x%x 0x%x
42552,3I,WLAN_MODULE_WAL -  WAL_DBGID_BRSSI_CONFIG  0x%x 0x%x 0x%x
42553,,WLAN_MODULE_WAL -  WAL_DBGID_CURRENT_BRSSI_AVE 
42554,,WLAN_MODULE_WAL -  WAL_DBGID_BCN_TX_COMP 
42555,4I,WLAN_MODULE_WAL -  WAL_DBGID_RX_REENTRY  0x%x 0x%x 0x%x 0x%x
42556,3I,WLAN_MODULE_WAL -  WAL_DBGID_SET_HW_CHAINMASK  0x%x 0x%x 0x%x
42557,2I,WLAN_MODULE_WAL -  WAL_DBGID_SET_HW_CHAINMASK_TXRX_STOP_FAIL  0x%x 0x%x
42558,2I,WLAN_MODULE_WAL -  WAL_DBGID_GET_HW_CHAINMASK  0x%x 0x%x
42559,,WLAN_MODULE_WAL -  WAL_DBGID_SMPS_DISABLE 
42560,2I,WLAN_MODULE_WAL -  WAL_DBGID_SMPS_ENABLE_HW_CNTRL  0x%x 0x%x
42561,2I,WLAN_MODULE_WAL -  WAL_DBGID_SMPS_SWSEL_CHAINMASK  0x%x 0x%x
42562,,WLAN_MODULE_WAL -  WAL_DBGID_SUSPEND 
42563,,WLAN_MODULE_WAL -  WAL_DBGID_RESUME 
42564,,WLAN_MODULE_WAL -  WAL_DBGID_PEER_TX_FAIL_CNT_THRES_EXCEEDED 
42565,3I,WAL - RX_FULL_REORDER Curr/Proc Idx=0x%x Reaped/Undelivered=0x%x Pdng/free=0x%x
42566,5I,WAL - WAL_DBGID_HCM_BIN   0x%x 0x%x 0x%x 0x%x 0x%x
42567,5I,WAL - WAL_DBGID_HCM_BIN_PENALIZE 0x%x 0x%x 0x%x 0x%x 0x%x
42568,5I,WAL - WAL_DBGID_HCM_BIN_DEPENALIZE 0x%x 0x%x 0x%x 0x%x 0x%x
42569,5I,WAL - WAL_DBGID_AST_UPDATE_WDS_ENTRY 0x%x 0x%x 0x%x 0x%x 0x%x
42570,5I,WAL - WAL_DBGID_PEER_EXT_STATS 0x%x 0x%x 0x%x 0x%x 0x%x
42571,5I,WAL - WAL_DBGID_TX_AC_BUFFER_SET 0x%x 0x%x 0x%x 0x%x 0x%x
42572,5I,WAL - WAL_DBGID_AST_ENTRY_EXIST 0x%x 0x%x 0x%x 0x%x 0x%x
42573,5I,WAL - WAL_DBGID_AST_ENTRY_FULL 0x%x 0x%x 0x%x 0x%x 0x%x
42574,5I,WLAN_MODULE_WAL -  WAL_DBGID_WMMAC_TXQ_STATUS ac=%d prev(bit4)/cur(bit0)_txq_status=0x%02x used_time_us=0x%x admitted_time_us=0x%x downgrade_type=%d (0=DEPRIO, 1=DROP)
42575,5I,WLAN_MODULE_WAL -  WAL_DBGID_PROLONGED_TX_PPDU_TOTAL_US t_ack=0x%x t_air=0x%x ack_wb_timestamp=0x%x ppdu_total_us=0x%x tx_ppdu_duration_us=0x%x
42576,5I,WLAN_MODULE_WAL -  WAL_DBGID_UPDATE_USED_TIME ppdu_total_us=0x%x prev_used_time_us=0x%x new_used_time_us=0x%x admitted_time_us=0x%x tx_status=%d(0=OK, 1=XRETRY,4=INITIALIZATION)
42577,5I,WLAN_MODULE_WAL -  WAL_DBGID_PAST_WB_ACK_TIMESTAMP t_ack=0x%x t_air=0x%x ack_wb_timestamp=0x%x ppdu_total_us=0x%x tx_status=%d(0=OK, 1=XRETRY, 2=DROP, 3=FILTERED)
42578,4I,WLAN_MODULE_WAL - WAL_DBGID_WMMAC_ADD_DEL_TSPEC 0x%x 0x%x 0x%x 0x%x
42579,4I,WLAN_MODULE_WAL - WAL_DBGID_WMMAC_TIMER_EXPIRY 0x%x 0x%x 0x%x 0x%x
42580,4I,WLAN_MODULE_WAL - WAL_DBGID_WMMAC_PARAMS 0x%x 0x%x 0x%x 0x%x
42581,,WLAN_MODULE_WAL -  WAL_DBGID_DEFINITION_END 
43008,,WAL_MODULE_DE
43520,,WLAN_MODULE_PCIELP
44032,2I,RTT -  RTT_CALL_FLOW  fn = %d ts = %d
44033,,RTT -  RTT_REQ_SUB_TYPE 
44034,2I,RTT -  RTT_MEAS_REQ_HEAD  req_id = %d sta_num = %d
44035,2I,RTT -  RTT_MEAS_REQ_BODY  control_inf = 0x%x meas_inf = 0x%x
44038,2I,RTT -  RTT_INIT_GLOBAL_STATE  init_idx = %d reason = %d
44040,4I,RTT -  RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x
44042,I,RTT -  RTT_ERROR_REPORT  err_id = %d
44043,,RTT -  RTT_TIMER_STOP 
44044,3I,RTT -  RTT_SEND_TM_FRAME  tkn = %d follow_tkn = %d tx_bw = %d
44045,I,RTT -  RTT_V3_RESP_CNT  number = %d
44046,,RTT -  RTT_V3_RESP_FINISH 
44047,2I,RTT -  RTT_CHANNEL_SWITCH_REQ  duration = %d channel = %d
44048,4I,RTT -  RTT_CHANNEL_SWITCH_GRANT  ev_id = %d p_chnl_switch_ctxt = 0x%x p_owner = 0x%x p_rtt_ctxt = 0x%x
44049,,RTT -  RTT_CHANNEL_SWITCH_COMPLETE 
44050,,RTT -  RTT_CHANNEL_SWITCH_PREEMPT 
44051,,RTT -  RTT_CHANNEL_SWITCH_STOP 
44052,,RTT -  RTT_TIMER_START 
44544,,WLAN_MODULE_RESOURCE -  RESOURCE_DBGID_DEFINITION_START 
44545,4I,RESOURCE -  RESOURCE_PEER_ALLOC  mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x usage_count = %d peer_type = %d
44546,3I,RESOURCE -  RESOURCE_PEER_FREE  mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x usage_count = %d
44547,4I,RESOURCE -  RESOURCE_PEER_ALLOC_WAL_PEER  mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x peer_type = %d status = %d
44548,2I,RESOURCE -  RESOURCE_PEER_NBRHOOD_MGMT_ALLOC  nbrhood_peers_ctxt = 0x%x var2 = %d
44549,3I,RESOURCE -  RESOURCE_PEER_NBRHOOD_MGMT_INFO  nbrhood_peers_ctxt/mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x num_valid_peers = %d
44550,,WLAN_MODULE_RESOURCE -  RESOURCE_DBGID_DEFINITION_END 
45056,I,WLAN_MODULE_DCS -  WLAN_DCS_DBGID_INIT  0x%x
45057,I,WLAN_MODULE_DCS -  WLAN_DCS_DBGID_WMI_CWINT  0x%x
45058,I,WLAN_MODULE_DCS -  WLAN_DCS_DBGID_TIMER  0x%x
45059,I,WLAN_MODULE_DCS -  WLAN_DCS_DBGID_CMDG  0x%x
45060,I,WLAN_MODULE_DCS -  WLAN_DCS_DBGID_CMDS  0x%x
45061,,WLAN_MODULE_DCS -  WLAN_DCS_DBGID_DINIT 
45568,,WLAN_MODULE_CACHEMGR
46080,4I,WLAN_MODULE_ANI -  ANI_DBGID_POLL   listen_time 0x%x 0x%x 0x%x 0x%x
46084,3I,WLAN_MODULE_ANI -  ANI_DBGID_RESET  resetFlags 0x%x resetCause 0x%x curChan 0x%x
46086,5I,WLAN_MODULE_ANI -  ANI_DBGID_OFDM_LEVEL  0x%x 0x%x 0x%x 0x%x 0x%x
46087,4I,WLAN_MODULE_ANI -  ANI_DBGID_CCK_LEVEL  0x%x 0x%x 0x%x 0x%x
46092,1I,WLAN_MODULE_ANI -  ANI_DBGID_ENABLE  anienable 0x%x 
46093,2I,WLAN_MODULE_ANI -  ANI_DBGID_CURRENT_LEVEL  ofdm_level = 0x%x  cck_level = 0x%x
46592,,WLAN_MODULE_P2P -  P2P_DBGID_DEFINITION_START 
46593,4I,WLAN_MODULE_P2P -  P2P_DEV_REGISTER  0x%x 0x%x 0x%x 0x%x
46594,4I,WLAN_MODULE_P2P -  P2P_HANDLE_NOA  0x%x 0x%x 0x%x 0x%x
46595,5I,WLAN_MODULE_P2P -  P2P_UPDATE_SCHEDULE_OPPS  0x%x 0x%x 0x%x 0x%x 0x%x
46596,4I,WLAN_MODULE_P2P -  P2P_UPDATE_SCHEDULE  duration = %d interval = %d start_time = %d type_count = %d
46597,2I,WLAN_MODULE_P2P -  P2P_UPDATE_START_TIME  curr_GOTSF32 = %d curr_FreeTSF = %d
46598,,WLAN_MODULE_P2P -  P2P_UPDATE_START_TIME_DIFF_TSF32 
46599,2I,WLAN_MODULE_P2P -  P2P_UPDATE_START_TIME_FINAL  0x%x 0x%x
46600,2I,WLAN_MODULE_P2P -  P2P_SETUP_SCHEDULE_TIMER  0x%x 0x%x
46601,4I,WLAN_MODULE_P2P -  P2P_PROCESS_SCHEDULE_AFTER_CALC  0x%x 0x%x 0x%x 0x%x
46602,3I,WLAN_MODULE_P2P -  P2P_PROCESS_SCHEDULE_STARTED_TIMER  0x%x 0x%x 0x%x
46603,,WLAN_MODULE_P2P -  P2P_CALC_SCHEDULES_FIRST_CALL_ALL_NEXT_EVENT 
46604,4I,WLAN_MODULE_P2P -  P2P_CALC_SCHEDULES_FIRST_VALUE  0x%x 0x%x 0x%x 0x%x
46605,3I,WLAN_MODULE_P2P -  P2P_CALC_SCHEDULES_EARLIEST_NEXT_EVENT  0x%x 0x%x 0x%x
46606,,WLAN_MODULE_P2P -  P2P_CALC_SCHEDULES_SANITY_COUNT 
46607,3I,WLAN_MODULE_P2P -  P2P_CALC_SCHEDULES_CALL_ALL_NEXT_EVENT_FROM_WHILE_LOOP  0x%x 0x%x 0x%x 
46608,I,WLAN_MODULE_P2P -  P2P_CALC_SCHEDULES_TIMEOUT_1  0x%x
46609,I,WLAN_MODULE_P2P -  P2P_CALC_SCHEDULES_TIMEOUT_2  0x%x
46610,I,WLAN_MODULE_P2P -  P2P_FIND_ALL_NEXT_EVENTS_REQ_EXPIRED  0x%x
46611,I,WLAN_MODULE_P2P -  P2P_FIND_ALL_NEXT_EVENTS_REQ_ACTIVE  0x%x
46612,I,WLAN_MODULE_P2P -  P2P_FIND_NEXT_EVENT_REQ_NOT_STARTED  0x%x
46613,2I,WLAN_MODULE_P2P -  P2P_FIND_NEXT_EVENT_REQ_COMPLETE_NON_PERIODIC  0x%x 0x%x
46614,2I,WLAN_MODULE_P2P -  P2P_FIND_NEXT_EVENT_IN_MID_OF_NOA  0x%x 0x%x
46615,2I,WLAN_MODULE_P2P -  P2P_FIND_NEXT_EVENT_REQ_COMPLETE  0x%x 0x%x
46616,3I,WLAN_MODULE_P2P -  P2P_SCHEDULE_TIMEOUT  0x%x 0x%x 0x%x
46617,I,WLAN_MODULE_P2P -  P2P_CALC_SCHEDULES_ENTER  0x%x
46618,I,WLAN_MODULE_P2P -  P2P_PROCESS_SCHEDULE_ENTER  0x%x
46619,5I,WLAN_MODULE_P2P -  P2P_FIND_ALL_NEXT_EVENTS_INDIVIDUAL_REQ_AFTER_CHANGE  0x%x 0x%x 0x%x 0x%x 0x%x
46620,,WLAN_MODULE_P2P -  P2P_FIND_ALL_NEXT_EVENTS_INDIVIDUAL_REQ_BEFORE_CHANGE 
46621,I,WLAN_MODULE_P2P -  P2P_FIND_ALL_NEXT_EVENTS_ENTER  0x%x
46622,I,WLAN_MODULE_P2P -  P2P_FIND_NEXT_EVENT_ENTER  0x%x
46623,3I,WLAN_MODULE_P2P -  P2P_NOA_GO_PRESENT  0x%x 0x%x 0x%x
46624,2I,WLAN_MODULE_P2P -  P2P_NOA_GO_ABSENT  0x%x 0x%x
46625,4I,WLAN_MODULE_P2P -  P2P_GO_NOA_NOTIF  0x%x 0x%x 0x%x 0x%x
46626,I,WLAN_MODULE_P2P -  P2P_GO_TBTT_OFFSET  0x%x
46627,4I,WLAN_MODULE_P2P -  P2P_GO_GET_NOA_INFO  0x%x 0x%x 0x%x 0x%x
46628,4I,WLAN_MODULE_P2P -  P2P_GO_ADD_ONE_SHOT_NOA  0x%x 0x%x 0x%x 0x%x
46629,4I,WLAN_MODULE_P2P -  P2P_GO_GET_NOA_IE  0x%x 0x%x 0x%x 0x%x
46630,4I,WLAN_MODULE_P2P -  P2P_GO_BCN_TX_COMP  0x%x 0x%x 0x%x 0x%x
46631,,WLAN_MODULE_P2P -  P2P_DBGID_DEFINITION_END 
47104,,WLAN_MODULE_CSA -  CSA_DBGID_DEFINITION_START 
47105,I,CSA -  CSA_OFFLOAD_POOL_INIT csa_ofld=0x%x
47106,I,CSA -  CSA_OFFLOAD_REGISTER_VDEV vdev_mode=0x%x
47107,I,CSA -  CSA_OFFLOAD_DEREGISTER_VDEV csa_ofld=0x%x
47108,,CSA -  CSA_DEREGISTER_VDEV_ERROR 
47109,4I,CSA -  CSA_OFFLOAD_BEACON_RECEIVED  mac addr:0x%x :0x%x :0x%x :0x%x
47110,I,CSA -  CSA_OFFLOAD_BEACON_CSA_RECV  tbtt_cnt=0x%x
47111,I,CSA -  CSA_OFFLOAD_CSA_RECV_ERROR_IE  tbtt_cnt=0x%x
47112,2I,CSA -  CSA_OFFLOAD_CSA_TIMER_ERROR  csa_proc/bcn_tsf=0x%x curr_tsf=0x%x
47113,2I,CSA -  CSA_OFFLOAD_CSA_TIMER_EXP  csa_proc=0x%x curr_tsf=0x%x
47114,I,CSA -  CSA_OFFLOAD_WMI_EVENT_ERROR  csa_proc=0x%x
47115,I,CSA -  CSA_OFFLOAD_WMI_EVENT_SENT  csa_proc=0x%x
47116,2I,CSA -  CSA_OFFLOAD_WMI_CHANSWITCH_RECV  cur_ch=0x%x new_ch=0x%x
47117,,WLAN_MODULE_CSA -  CSA_DBGID_DEFINITION_END
47616,2I,WLAN_MODULE_NLO - NLO_DBGID_SSID_TO_BE_SCANNED_LIST  0x%x 0x%x
47617,I,WLAN_MODULE_NLO - NLO_DBGID_SSID_TO_BE_SKIPPED_LIST 0x%x
48128,,WLAN_MODULE_CHATTER -  WLAN_CHATTER_DBGID_DEFINITION_START 
48129,,CHATTER -  WLAN_CHATTER_ENTER 
48130,,CHATTER -  WLAN_CHATTER_EXIT 
48131,I,CHATTER -  WLAN_CHATTER_FILTER_HIT  filter_id = 0x%x
48132,,CHATTER -  WLAN_CHATTER_FILTER_MISS 
48133,I,CHATTER -  WLAN_CHATTER_FILTER_FULL  num_of_rules = 0x%x
48134,2I,CHATTER -  WLAN_CHATTER_FILTER_TM_ADJ  filter_id = 0x%x max_coalescing_delay = 0x%x
48135,I,CHATTER -  WLAN_CHATTER_BUFFER_FULL  store_cnt = 0x%x
48136,,CHATTER -  WLAN_CHATTER_TIMEOUT 
48137,4I,CHATTER -  WLAN_CHATTER_MC_FILTER_ADD  vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x status = 0x%x
48138,4I,CHATTER -  WLAN_CHATTER_MC_FILTER_DEL  vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x status = 0x%x
48139,3I,CHATTER -  WLAN_CHATTER_MC_FILTER_ALLOW  vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x
48140,3I,CHATTER -  WLAN_CHATTER_MC_FILTER_DROP  vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x
48141,2I,CHATTER -  WLAN_CHATTER_COALESCING_FILTER_ADD  num_of_rules/add filter status = 0x%x new_filter_id/num_of_rules = 0x%x
48142,,CHATTER -  WLAN_CHATTER_COALESCING_FILTER_DEL 
48143,,WLAN_MODULE_CHATTER -  WLAN_CHATTER_DBGID_DEFINITION_END 
48640,,WLAN_MODULE_WOW -  WOW_DBGID_DEFINITION_START 
48641,3I,WOW -  WOW_ENABLE_CMDID  recv_cmd/operate_state = 0x%x tx_pending_cnt/is_block/wake_reason = 0x%x wow_allow = 0x%x
48642,3I,WOW -  WOW_RECV_DATA_PKT  tgt_ip = 0x%x src_ip = 0x%x ops = 0x%x
48643,3I,WOW -  WOW_WAKE_HOST_DATA   length/store_faliure = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x
48644,I,WOW -  WOW_RECV_MGMT  frame_type = 0x%x
48645,,WOW -  WOW_WAKE_HOST_MGMT 
48646,,WOW -  WOW_RECV_EVENT 
48647,6I,WOW -  WOW_WAKE_HOST_EVENT  0x%x 0x%x 0x%x 0x%x 0x%x 0x%x
48648,,WOW -  WOW_INIT 
48649,I,WOW -  WOW_RECV_MAGIC_PKT  0x%x
48650,I,WOW -  WOW_RECV_BITMAP_PATTERN  pattern_id = 0x%x
48651,I,WOW -  WOW_AP_VDEV_DISALLOW  allow_status = 0x%x
48652,I,WOW -  WOW_STA_VDEV_DISALLOW  0x%x
48653,I,WOW -  WOW_P2PGO_VDEV_DISALLOW  0x%x
48654,4I,WOW -  WOW_NS_OFLD_ENABLE  ipv6_addr_31_0 = 0x%x ipv6_addr_63_32 = 0x%x ipv6_addr_95_64 = 0x%x ipv6_addr_127_96 = 0x%x
48655,I,WOW -  WOW_ARP_OFLD_ENABLE  ip_addr = 0x%x
48656,,WOW -  WOW_NS_ARP_OFLD_DISABLE 
48657,4I,WOW -  WOW_NS_RECEIVED  ipv6_addr_31_0 = 0x%x ipv6_addr_63_32 = 0x%x ipv6_addr_95_64 = 0x%x ipv6_addr_127_96 = 0x%x
48658,4I,WOW -  WOW_NS_REPLIED  ipv6_addr_31_0 = 0x%x ipv6_addr_63_32 = 0x%x ipv6_addr_95_64 = 0x%x ipv6_addr_127_96 = 0x%x
48659,I,WOW -  WOW_ARP_RECEIVED  ip_addr = 0x%x
48660,I,WOW -  WOW_ARP_REPLIED  ip_addr = 0x%x
48661,3I,WOW -  WOW_BEACON_OFFLOAD_TX  completion_status = 0x%x bcn_pending_count = 0x%x bcn_buf_initialized = 0x%x
48662,,WOW -  WOW_BEACON_OFFLOAD_CFG 
48663,2I,WOW -  WOW_IBSS_VDEV_ALLOW status = 0x%x num_peer = 0x%x 
48664,,WLAN_MODULE_WOW -  WOW_DBGID_DEFINITION_END 
49152,,WLAN_MODULE_WAL_VDEV
49664,,WLAN_MODULE_WAL_PDEV
50176,,WLAN_MODULE_TEST
50688,,WLAN_MODULE_STA_SMPS -  STA_SMPS_DBGID_DEFINITION_START 
50689,,STA_SMPS -  STA_SMPS_DBGID_CREATE_PDEV_INSTANCE 
50690,I,STA_SMPS -  STA_SMPS_DBGID_CREATE_VIRTUAL_CHAN_INSTANCE  vc_handle = 0x%x
50691,I,STA_SMPS -  STA_SMPS_DBGID_DELETE_VIRTUAL_CHAN_INSTANCE  vc_handle = 0x%x
50692,I,STA_SMPS -  STA_SMPS_DBGID_CREATE_STA_INSTANCE  sta_handle = 0x%x
50693,I,STA_SMPS -  STA_SMPS_DBGID_DELETE_STA_INSTANCE  sta_handle = 0x%x
50694,I,STA_SMPS -  STA_SMPS_DBGID_VIRTUAL_CHAN_SMPS_START  vc_handle = 0x%x
50695,I,STA_SMPS -  STA_SMPS_DBGID_VIRTUAL_CHAN_SMPS_STOP  vc_handle = 0x%x
50696,,STA_SMPS -  STA_SMPS_DBGID_SEND_SMPS_ACTION_FRAME 
50697,I,STA_SMPS -  STA_SMPS_DBGID_HOST_FORCED_MODE  event = 0x%x
50698,I,STA_SMPS -  STA_SMPS_DBGID_FW_FORCED_MODE  event = 0x%x
50699,I,STA_SMPS -  STA_SMPS_DBGID_RSSI_THRESHOLD_CROSSED  rssi_upper_threshold/rssi_lower_threshold = 0x%x
50700,3I,STA_SMPS -  STA_SMPS_DBGID_SMPS_ACTION_FRAME_COMPLETION  sm_power_control = 0x%x last_frame_sm_pwr_ctrl = 0x%x completion_status = 0x%x
50701,,STA_SMPS -  STA_SMPS_DBGID_DTIM_EBT_EVENT_CHMASK_UPDATE 
50702,3I,STA_SMPS -  STA_SMPS_DBGID_DTIM_CHMASK_UPDATE  curr_brssi = 0x%x rx_chain_mask = 0x%x arb_dtim_chainmask = 0x%x
50703,,STA_SMPS -  STA_SMPS_DBGID_DTIM_BEACON_EVENT_CHMASK_UPDATE 
50704,2I,STA_SMPS -  STA_SMPS_DBGID_DTIM_POWER_STATE_CHANGE  cur_power_state = 0x%x new_power_state = 0x%x
50705,4I,STA_SMPS -  STA_SMPS_DBGID_DTIM_CHMASK_UPDATE_SLEEP  tx_chain_mask = 0x%x rx_chain_mask = 0x%x orig_rx_chainmask = 0x%x arb_dtim_rx_chainmask = 0x%x
50706,3I,STA_SMPS -  STA_SMPS_DBGID_DTIM_CHMASK_UPDATE_AWAKE  tx_chain_mask = 0x%x rx_chain_mask = 0x%x orig_rx_chainmask = 0x%x
50706,,WLAN_MODULE_STA_SMPS -  STA_SMPS_DBGID_DEFINITION_END 
51200,,WLAN_MODULE_SWBMISS -  SWBMISS_DBGID_DEFINITION_START 
51201,5I,SWBMISS -  SWBMISS_ENABLED  vdev_id = 0x%x module_id = 0x%x bmiss_disable_bitmap_63_32 0x%x bmiss_disable_bitmap_31_0 = 0x%x curr_bmiss_bcnt = 0x%x
51202,5I,SWBMISS -  SWBMISS_DISABLED  vdev_id = 0x%x module_id = 0x%x bmiss_disable_bitmap_63_32 0x%x bmiss_disable_bitmap_31_0 = 0x%x curr_bmiss_bcnt = 0x%x
51203,,WLAN_MODULE_SWBMISS -  SWBMISS_DBGID_DEFINITION_END 
51712,,WLAN_MODULE_WMMAC
52224,,WLAN_MODULE_TDLS -  TDLS_DBGID_DEFINITION_START
52225,,TDLS -  TDLS_DBGID_VDEV_CREATE Tdls2:
52226,,TDLS -  TDLS_DBGID_VDEV_DELETE Tdls3:
52227,4I,TDLS -  TDLS_DBGID_ENABLED_PASSIVE  Tdls4:magic# = 0x%x fn_id = 0x%x step = 0x%x wmi_value = 0x%x
52228,4I,TDLS -  TDLS_DBGID_ENABLED_ACTIVE  Tdls5:magic# = 0x%x fn_id = 0x%x step = 0x%x wmi_value = 0x%x
52229,,TDLS -  TDLS_DBGID_DISABLED Tdls6:
52230,4I,TDLS -  TDLS_DBGID_CONNTRACK_TIMER  Tdls7:step# = 0x%x val1 = 0x%x val2 = 0x%x val3 = 0x%x
52231,2I,TDLS -  TDLS_DBGID_WAL_SET  Tdls8:param_type = %d value = 0x%x
52232,I,TDLS -  TDLS_DBGID_WAL_GET  Tdls9:param_type = %d
52233,5I,TDLS -  TDLS_DBGID_WAL_PEER_UPDATE_SET  Tdls10:step = 0x%x val1 = 0x%x val2 = 0x%x val3 = 0x%x vl4 = 0x%x
52234,3I,TDLS -  TDLS_DBGID_WAL_PEER_UPDATE_EVT  Tdls11:mac47to32= 0x%x mac31to0 = 0x%x reason = 0x%x
52235,I,TDLS -  TDLS_DBGID_WAL_VDEV_CREATE  Tdls12:step = 0x%x
52236,,TDLS -  TDLS_DBGID_WAL_VDEV_DELETE Tdls13:
52237,5I,TDLS -  TDLS_DBGID_WLAN_EVENT  Tdls14:val1 = 0x%x val2 = 0x%x val3 = 0x%x val4 = 0x%x val5 = 0x%x
52238,7I,TDLS -  TDLS_DBGID_WLAN_PEER_UPDATE_SET  Tdls15:val1 = 0x%x val2 = 0x%x val3 = 0x%x val4 = 0x%x val5 = 0x%x val6 = 0x%x val7 = 0x%x
52239,5I,TDLS -  TDLS_DBGID_PEER_EVT_DRP_THRESH  Tdls16:mac47to32 = 0x%x tx_threshold = %d tx_count = %d tx_avg = %d rx_avg = %d
52240,,TDLS -  TDLS_DBGID_PEER_EVT_DRP_RATE Tdls17:
52241,5I,TDLS -  TDLS_DBGID_PEER_EVT_DRP_RSSI  Tdls18:step = 0x%x mac47to32 = 0x%x mac31to0 = 0x%x new_rssi_threshold = %d peer_rssi = %d
52242,5I,TDLS -  TDLS_DBGID_PEER_EVT_DISCOVER  Tdls19:step = 0x%x mac47to32 = 0x%x mac31to0 = 0x%x tx_avg = %d discovery_threshold = %d
52243,4I,TDLS -  TDLS_DBGID_PEER_EVT_DELETE  Tdls20:val1 = 0x%x val2 = 0x%x val3 = 0x%x val4 = 0x%x
52244,5I,TDLS -  TDLS_DBGID_PEER_CAP_UPDATE  Tdls21:val1 = 0x%x val2 = 0x%x val3 = 0x%x val4 = 0x%x val5 = 0x%x
52245,5I,TDLS -  TDLS_DBGID_UAPSD_SEND_PTI_FRAME  Tdls22:magic# = 0x%x fn_id = 0x%x val1 = 0x%x val2 = 0x%x val3 = 0x%x
52246,4I,TDLS -  TDLS_DBGID_UAPSD_SEND_PTI_FRAME2PEER  Tdls23:magic# = 0x%x fn_id = 0x%x step = 0x%x value = 0x%x
52247,,TDLS -  TDLS_DBGID_UAPSD_START_PTR_TIMER Tdls24:
52248,5I,TDLS -  TDLS_DBGID_UAPSD_CANCEL_PTR_TIMER  Tdls25:magic# = 0x%x fn_id = 0x%x step = 0x%x val1 = 0x%x val2 = 0x%x
52249,4I,TDLS -  TDLS_DBGID_UAPSD_PTR_TIMER_TIMEOUT  Tdls26:val1 = 0x%x val2 = 0x%x val3 = 0x%x val4 = 0x%x
52250,5I,TDLS -  TDLS_DBGID_UAPSD_STA_PS_EVENT_HANDLER  Tdls27:val1 = 0x%x val2 = 0x%x val3 = 0x%x val4 = 0x%x val5 = 0x%x
52251,5I,TDLS -  TDLS_DBGID_UAPSD_PEER_EVENT_HANDLER  Tdls28:magic# = 0x%x fn_id = 0x%x val1 = 0x%x val2 = 0x%x val3 = 0x%x
52252,5I,TDLS -  TDLS_DBGID_UAPSD_PS_DEFAULT_SETTINGS  Tdls29:magic# = 0x%x fn_id = 0x%x assoc_id = %d uapsd_trigger_tids = 0x%x default_legacy_ac = 0x%x
52253,5I,TDLS -  TDLS_DBGID_UAPSD_GENERIC  Tdls30:magic# = 0x%x fn_id = 0x%x step = 0x%x val1 = 0x%x val2 = 0x%x
52736,,WLAN_MODULE_HB -  WLAN_HB_DBGID_DEFINITION_START 
52737,,WLAN_MODULE_HB -  WLAN_HB_DBGID_INIT 
52738,I,WLAN_MODULE_HB -  WLAN_HB_DBGID_TCP_GET_TXBUF_FAIL  0x%x 
52739,2I,WLAN_MODULE_HB -  WLAN_HB_DBGID_TCP_SEND_FAIL  0x%x 0x%x
52740,,WLAN_MODULE_HB -  WLAN_HB_DBGID_BSS_PEER_NULL 
52741,I,WLAN_MODULE_HB -  WLAN_HB_DBGID_UDP_GET_TXBUF_FAIL  0x%x 
52742,2I,WLAN_MODULE_HB -  WLAN_HB_DBGID_UDP_SEND_FAIL  0x%x 0x%x
52743,4I,WLAN_MODULE_HB -  WLAN_HB_DBGID_WMI_CMD_INVALID_PARAM  0x%x 0x%x 0x%x 0x%x
52744,3I,WLAN_MODULE_HB -  WLAN_HB_DBGID_WMI_CMD_INVALID_OP  0x%x 0x%x 0x%x
52745,2I,WLAN_MODULE_HB -  WLAN_HB_DBGID_WOW_NOT_ENTERED  0x%x 0x%x
52746,,WLAN_MODULE_HB -  WLAN_HB_DBGID_ALLOC_SESS_FAIL 
52747,2I,WLAN_MODULE_HB -  WLAN_HB_DBGID_CTX_NULL  0x%x 0x%x
52748,I,WLAN_MODULE_HB -  WLAN_HB_DBGID_CHKSUM_ERR 0x%x 
52749,2I,WLAN_MODULE_HB -  WLAN_HB_DBGID_UDP_TX  0x%x 0x%x
52750,2I,WLAN_MODULE_HB -  WLAN_HB_DBGID_TCP_TX  0x%x 0x%x
52751,,WLAN_MODULE_HB -  WLAN_HB_DBGID_DEFINITION_END 
53248,,WLAN_MODULE_TXBF -  TXBFEE_DBGID_START 
53249,3I,TXBF -  TXBFEE_DBGID_NDPA_RECEIVED  sInfo0=0x%x sInfo1=0x%x Token=0x%x
53250,2I,TXBF -  TXBFEE_DBGID_HOST_CONFIG_TXBFEE_TYPE  SU=0x%x MU=0x%x
53251,,TXBF -  TXBFER_DBGID_SEND_NDPA 
53252,,TXBF -  TXBFER_DBGID_GET_NDPA_BUF_FAIL 
53253,,TXBF -  TXBFER_DBGID_SEND_NDPA_FAIL 
53254,,TXBF -  TXBFER_DBGID_GET_NDP_BUF_FAIL 
53255,,TXBF -  TXBFER_DBGID_SEND_NDP_FAIL 
53256,,TXBF -  TXBFER_DBGID_GET_BRPOLL_BUF_FAIL 
53257,,TXBF -  TXBFER_DBGID_SEND_BRPOLL_FAIL 
53258,,TXBF -  TXBFER_DBGID_HOST_CONFIG_CMDID 
53259,2I,TXBF -  TXBFEE_DBGID_HOST_CONFIG_CMDID  ID=0x%x Value=0x%x
53260,,TXBF -  TXBFEE_DBGID_ENABLE_UPLOAD_H 
53261,,TXBF -  TXBFEE_DBGID_UPLOADH_CV_TAG 
53262,,TXBF -  TXBFEE_DBGID_UPLOADH_H_TAG 
53263,,TXBF -  TXBFEE_DBGID_CAPTUREH_RECEIVED 
53264,,TXBF -  TXBFEE_DBGID_PACKET_IS_STEERED 
53265,,TXBF -  TXBFEE_UPLOADH_EVENT_ALLOC_MEM_FAIL 
53266,,TXBF -  TXBFEE_DBGID_SW_WAR_AID_ZERO 
53267,,WLAN_MODULE_TXBF -  TXBFEE_DBGID_END 
53760,,WLAN_MODULE_BATCH_SCAN
54272,,WLAN_MODULE_THERMAL_MGR -  THERMAL_MGR_DBGID_DEFINITION_START 
54273,2I,THERMAL_MGR -  THERMAL_MGR_NEW_THRESH low %d up %d 
54274,I,THERMAL_MGR -  THERMAL_MGR_THRESH_CROSSED %d
54275,,WLAN_MODULE_THERMAL_MGR -  THERMAL_MGR_DBGID_DEFINITION_END 
54784,,WLAN_MODULE_PHYERR_DFS -  WLAN_PHYERR_DFS_DBGID_DEFINITION_START 
54785,3I,PHYERR_DFS -  WLAN_PHYERR_DFS_PHYERR_INFO_CHAN_BUFLEN  chan=0x%x width=0x%x buf=0x%x
54786,4I,PHYERR_DFS -  WLAN_PHYERR_DFS_PHYERR_INFO_PPDU  ppdu_ts=0x%x chain0_rssi=0x%x chain1_rssi=0x%x rssi=0x%x
54787,4I,PHYERR_DFS -  WLAN_PHYERR_DFS_DBDID_RADAR_SUMMARY  pl_sidx=0x%x ts_ofst=0x%x dur=0xchain0_rssi%x is_chirp=0x%x
54788,3I,PHYERR_DFS -  WLAN_PHYERR_DFS_DBDID_SEARCH_FFT  peak_idx=0x%x peak_mag=0x%x str_bins=0x%x
54789,I,PHYERR_DFS -  WLAN_PHTERR_DFS_DBDID_FILTER_STATUS  filter_status=0x%x
54790,,WLAN_MODULE_PHYERR_DFS -  WLAN_PHYERR_DFS_DBGID_DEFINITION_END 
55296,,WLAN_MODULE_RMC -  RMC_DBGID_DEFINITION_START 
55297,2I,RMC -  RMC_CREATE_INSTANCE  pdev_hndl/vdev_ctxt_pool = 0x%x vdev = 0x%x
55298,I,RMC -  RMC_DELETE_INSTANCE  rmc_hndl = 0x%x
55299,4I,RMC -  RMC_LDR_SEL  mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x bcn_rssi = %d selected = %d
55300,,RMC -  RMC_NO_LDR 
55301,,RMC -  RMC_LDR_NOT_SEL 
55302,4I,RMC -  RMC_LDR_INF_SENT  peer/status = 0x%x mac_addr47to32 = 0x%x mac_addr31to0 = 0x%x cancellation = %d
55303,3I,RMC -  RMC_PEER_ADD  peer = 0x%x mac_addr47to32 = 0x%x mac_addr31to0 = 0x%x
55304,3I,RMC -  RMC_PEER_DELETE  peer = 0x%x mac_addr47to32 = 0x%x mac_addr31to0 = 0x%x
55305,,RMC -  RMC_PEER_UNKNOWN 
55306,I,RMC -  RMC_SET_MODE  enable_rmc = %d
55307,I,RMC -  RMC_SET_ACTION_PERIOD  period_ms = %d
55308,2I,RMC -  RMC_ACTION_FRAME_RX  var1 = 0x%x len/subtype = %d
55309,I,RMC -  RMC_WAL_EVENT_HANDLER  event_type = 0x%x
55310,5I,RMC -  RMC_BLACKLIST_PEER  mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x bl_ts = 0x%x bl_last_bcn_rssi = %d bl_avg_bcn_rssi = %d
55311,5I,RMC -  RMC_WHITELIST_PEER  mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x diff_us = %d curr_rssi = %d bl_rssi = %d
55312,3I,RMC -  RMC_PEER_BCN_INFO  mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x bcn_rssi = %d
55313,,WLAN_MODULE_RMC -  RMC_DBGID_DEFINITION_END 
55808,,WLAN_MODULE_STATS -  WLAN_STATS_DBGID_DEFINITION_START 
55809,I,STATS -  WLAN_STATS_DBGID_EST_LINKSPEED_VDEV_EN_DIS  0x%x
55810,3I,STATS -  WLAN_STATS_DBGID_EST_LINKSPEED_CHAN_TIME_START  0x%x cur_power_state 0x%x new_power_state 0x%x
55811,4I,STATS -  WLAN_STATS_DBGID_EST_LINKSPEED_CHAN_TIME_END  chan_mhz 0x%x chan_mhz 0x%x busy_time_us 0x%x accu_idle_dur_us 0x%x
55812,3I,STATS -  WLAN_STATS_DBGID_EST_LINKSPEED_CALC  0x%x 0x%x 0x%x
55813,2I,STATS -  WLAN_STATS_DBGID_EST_LINKSPEED_UPDATE_HOME_CHAN  chan_mhz 0x%x home_chan_added 0x%x
55814,,WLAN_MODULE_STATS -  WLAN_STATS_DBGID_DEFINITION_END 
56320,3I,NAN_MODULE_ID -  NAN_DBGID_START 
56321,5I,NAN - FUNC_BEGIN: mod %u line %u:0x%x 0x%x 0x%x
56322,5I,NAN - FUNC_END: mod %u  line %u: 0x%x 0x%x 0x%x
56323,5I,NAN - MAIN_DEBUG: mod %u  line %u: 0x%x 0x%x 0x%x
56324,5I,NAN - MAC_DEBUG: mod %u  line%u: 0x%x 0x%x 0x%x
56325,5I,NAN - BLOOM_FILTER_DEBUG: mod %u  line %u: 0x%x 0x%x 0x%x
56326,5I,NAN - MAC_ADDR: mod %u  line %u: 0x%x 0x%x 0x%x
56327,5I,NAN - PARAM_UPDATED: mod %u  line %u: 0x%x 0x%x 0x%x
56328,5I,NAN - NULL_PTR: mod %u  line %u: 0x%x 0x%x 0x%x
56329,5I,NAN - INVALID_FUNC_ARG: mod %u  line %u: 0x%x 0x%x 0x%x
56330,5I,NAN - INVALID_MSG_PARAM: mod %u  line %u: 0x%x 0x%x 0x%x
56331,5I,NAN - MISSING_MSG_PARAM: mod %u  line %u: 0x%x 0x%x 0x%x
56332,5I,NAN - DEPRECATED_MSG_PARAM: mod %u  line %u: 0x%x 0x%x 0x%x
56333,5I,NAN - UNSUPPORTED_MSG_PARAM: mod %u  line %u: 0x%x 0x%x 0x%x
56334,5I,NAN - INVALID_PKT_DATA: mod %u  line %u: 0x%x 0x%x 0x%x
56335,5I,NAN - LOG_PKT_DATA: mod %u  line %u: 0x%x 0x%x 0x%x
56336,5I,NAN - INVALID_VALUE: mod %u  line %u: 0x%x 0x%x 0x%x
56337,5I,NAN - INVALID_OPERATION: mod %u  line %u: 0x%x 0x%x 0x%x
56338,5I,NAN - INVALID_STATE: mod %u  line %u: 0x%x 0x%x 0x%x
56339,5I,NAN - FUNCTION_ENABLED: mod %u, line %u: 0x%x 0x%x 0x%x
56340,5I,NAN - FUNCTION_DISABLED: mod %u  line %u: 0x%x 0x%x 0x%x
56341,5I,NAN - INVALID_FUNCTION_STATE: mod %u  line %u: 0x%x 0x%x 0x%x
56342,5I,NAN - READ_ERROR: mod %u  line %u: 0x%x 0x%x 0x%x
56343,5I,NAN - WRITE_ERROR: mod %u  line %u: 0x%x 0x%x 0x%x
56344,5I,NAN - RECEIVE_ERROR: mod %u  line %u: 0x%x 0x%x 0x%x
56345,5I,NAN - TRANSMIT_ERROR: mod %u  line %u: 0x%x 0x%x 0x%x
56346,5I,NAN - PARSE_ERROR: mod %u  line %u: 0x%x 0x%x 0x%x
56347,5I,NAN - RES_ALLOC_ERROR: mod %u  line %u: 0x%x 0x%x 0x%x
56348,,NAN - ENABLED
56349,,NAN - DISABLED
56350,,NAN - CONFIG_RESTORED 
56351,I,NAN - SDF_QUEUED: count %u
56352,2I,NAN - TW_CHANGED: %u -> %u
56353,2I,NAN [==================================> DW_START (pri=%u  5g=%u)
56354,,NAN <==================================] DW_STOP
56355,2I,NAN - CLUSTER_ID_CHANGED: 0x%04x -> 0x%04x
56356,3I,NAN - WMI_CMD_RECEIVED: cmd=0x%x  buffer=%p  length=%u
56357,4I,NAN - WMI_EVT_SENT: pEventPkt=%p  pEventBuf=%p  eventSize=%u  dataSize=%u
56358,3I,NAN - TLV_READ: type %u  length %u  readLen %u
56359,3I,NAN - TLV_WRITE: type %u  length %u  writeLen %u
56360,3I,NAN - PUBSUB_UPDATED: handle %u
56361,I,NAN - PUBSUB_REMOVE_DEFERED: handle %u
56362,I,NAN - PUBSUB_REMOVE_PENDING: handle %u
56363,I,NAN - PUBSUB_REMOVED: handle %u
56364,3I,NAN - PUBSUB_PROCESSED: handle %u  status %u  value %u 
56365,I8b2I,NAN - PUBSUB_MATCHED: handle %u  svcId %02X:%02X:%02X:%02X:%02X:%02X  inId %u  reqId %u  svcCtrl 0x%02x  len %u
56366,2I,NAN - PUBSUB_PREPARED: handle %u  flags 0x%X
56367,2I8b,NAN - PUBSUB_FOLLOWUP_TRANSMIT: handle %u  matchHandle 0x%04X  svcId %02X:%02X:%02X:%02X:%02X:%02X  reqId %u
56368,2I8b,NAN - PUBSUB_FOLLOWUP_RECEIVED: handle %u  matchHandle 0x%04X  macAddr %02X:%02X:%02X:%02X:%02X:%02X  inId %u  reqId %u
56369,4I,NAN - SUBSCRIBE_UNMATCH_TIMEOUT_UPDATE: xrefHandle %u  handle %u  Tp %u  Tn %u
56370,3I,NAN - SUBSCRIBE_MATCH_NEW: handle %u  match handle %u  timestamp %u
56371,3I,NAN - SUBSCRIBE_MATCH_REPEAT: handle %u  match handle %u  timestamp %u
56372,4I,NAN - SUBSCRIBE_MATCH_EXPIRED: xrefHandle %u  handle %u  match timestamp %u  timestamp %u
56373,4I,NAN - SUBSCRIBE_MATCH_LOG: handle %u  match handle %u  match timestamp %u  timestamp %u
56374,6b,NAN - SERVICE_ID_CREATED: %02X:%02X:%02X:%02X:%02X:%02X
56375,I,NAN - SD_ATTR_BUILT: size %u
56376,I,NAN - SERVICE_RSP_OFFSET: offset %u
56377,I,NAN - SERVICE_INFO_OFFSET: offset %u
56378,4I,NAN - CHREQ_CREATE: freq %u  interval %u  start_time 0x%08x  duration 0x%x
56379,4I,NAN - CHREQ_UPDATE: freq %u  interval %u  start_time 0x%08x  duration 0x%x
56380,4I,NAN - CHREQ_REMOVE: freq %u  interval %u  status %u
56381,3I,NAN - CHREQ_GRANT: freq %u  type %u  tsfLo 0x%08x
56382,3I,NAN - CHREQ_END: freq %u  type %u  tsfLo 0x%x
56383,3I,NAN - CHREQ_ERROR: freq %u  type %u  tsfLo 0x%08x
56384,5I,NAN - RX_CALLBACK: type 0x%X  lenth %u  currTsf 0x%08x  rssi %u  freq %u
56385,5I,NAN - TX_COMPLETE: type 0x%X  handle %p  buf %p  status %u  currTsf 0x%08x
56386,2I,NAN - TSF_TIMEOUT: currTsf 0x%08x  usecs %u
56387,2I,NAN - SYNC_START: clusterId 0x%04x (startedFlag %u) 
56388,I,NAN - SYNC_STOP: clusterId 0x%04x
56389,3I,NAN - NAN_SCAN: enable %u  type %u  rval %u
56390,I,NAN - NAN_SCAN_COMPLETE: type %u
56391,I,NAN - MPREF_CHANGE: new masterPref=%u
56392,2I,NAN - WARMUP_EXPIRE: masterPref=%u randomFactor=%u
56393,I,NAN - RANDOM_FACTOR_EXPIRE: new randomFactor=%u
56394,2I,NAN - DW_SKIP: currTsf 0x%08x  diff %08x
56395,2I,NAN - DB_SKIP: reason 0x%x  diff 0x%08x
56396,8bhhI,NAN - BEACON_RX: from %02x:%02x:%02x:%02x:%02x:%02x  RSSI %u  valid %u  cluster 0x%04x  BI %u  statusFlags 0x%08x
56397,3I,NAN - BEACON_TX (prepare): buf %p  len %u  rval %u
56398,5I,NAN - CLUSTER_MERGE: Merging to cluster 0x%04x [amRank=0x%08x_%08x  TS=0x%08x_%08x]
56399,3I,NAN - TEST_CMD_EXEC: 0x%x 0x%x 0x%x
56400,3I,NAN - APPLY_BEACON_TSF: timestamp=0x%08x_%08x  age=0x%08x
56401,2I,NAN - TSF_UPDATE: behind %u diff %u
56402,4I,NAN - SET_TSF: raw 0x%08x_%08x  nan 0x%08x_%08x
56403,4I,NAN - NEW_MASTERRANK: rank=0x%08x_%08x (mp=%d  rf=%d)
56404,4I,NAN - NEW_ANCHORMASTER: rank=0x%08x_%08x (mp=%d  rf=%d)
56405,4I,NAN - ANCHORMASTER_RECORD_UPDATE: rank=0x%08x_%08x HC=%d BTT=0x%08x
56406,4I,NAN - ANCHORMASTER_RECORD_EXPIRED: rank=0x%08x_%08x HC=%d BTT=0x%08x
56407,2I,NAN - BECOMING_ANCHORMASTER: reason=%u  transistionsToAM=%u
56408,3I,NAN - ROLE_CHANGE: %u -> %u (isFORCED=%u)
56409,I8h,NAN - SYNC_BEACON_DW_STATS: total rx %u  c1=(%u/%u/%u  %u) c2=(%u/%u/%u  %u)
56410,3I,NAN - RX_UNSUPPORTED_SDF_ATTR_ID: 0x%x 0x%x 0x%x
56411,I8b2I,NAN - PUBSUB_MATCHED_SKIPPED_SSI: handle %u  svcId %02X:%02X:%02X:%02X:%02X:%02X  inId %u  reqid %u  svcCtrl 0x%02x  len %u
56412,I,NAN - MATCH_FILTER_OFFSET: offset %u
56413,3I,NAN - TW_PARAMS: twSize=%u  n=%u  twIndex=%u
56414,3I,NAN - BEACON_SENDER: code 0x%x  idx %u  sender 0x%08x
56415,4I,NAN - TSF_DUMP: currTsf 0x%08x_%08x  nextDwTsf 0x%08x_%08x
56416,4I,NAN - FAW_CONFIG: chan %u  startSlot %u  numSlots %u  repeat %u
56417,I,NAN [----------------------------------> FAW_START (is5G %u)
56418,I,NAN <----------------------------------] FAW_END (%u)
56419,3I,NAN - CONFIG_PARAM_CHANGED: offset %d  0x%08x => 0x%08x
56420,,NAN - CONN_CAP_ATTR_CLEARED
56421,,NAN - POST_DISC_ATTR_CLEARED
56422,,NAN - VENDOR_SPECIFIC_ATTR_CLEARED
56423,I,NAN - WLAN_INFRA_MAP_CTRL_OFFSET: offset %u
56424,I,NAN - WLAN_INFRA_AI_BITMAP_OFFSET: offset %u
56425,I,NAN - WLAN_INFRA_DEVICE_ROLE_OFFSET: offset%u
56426,I,NAN - MESH_ID_OFFSET: offset %u
56427,5I,NAN - NAN_DBGID_SPARE_79: 0x%x 0x%x 0x%x 0x%x 0x%x
56428,5I,NAN - NAN_DBGID_SPARE_80: 0x%x 0x%x 0x%x 0x%x 0x%x
56429,5I,NAN - NAN_DBGID_SPARE_81: 0x%x 0x%x 0x%x 0x%x 0x%x
56430,5I,NAN - NAN_DBGID_SPARE_82: 0x%x 0x%x 0x%x 0x%x 0x%x
56431,5I,NAN - NAN_DBGID_SPARE_83: 0x%x 0x%x 0x%x 0x%x 0x%x
56432,5I,NAN -> API_MSG_HEADER: msgId %u  msgVersion %u  msgLen %u  handle %u  transId %u
56433,4b4b4b4b4b,NAN ->     MSG_DATA: %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X
56434,2I,NAN -  OTA_PKT_HEADER:  isTx %u  frameLength %u
56435,4b4b4b4b4b,NAN ->      PKT_DATA: %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X %02X
56436,5I,NAN -    Times: NAN TSF 0x%08x_%08x  hwRxTs 0x%08x  TS 0x%08x_%08x
56437,2h4I,NAN -    Attrs: [mpref=%d  randf=%d]  [amRank=0x%08x_%08x amHC=%d amBTT=%08x]
56438,I,NAN -    SID Attr: contains %d IDs
56439,4I,NAN -    VSA Attr: oui %02x:%02x:%02x  bodyLen %u
56440,hh4b4b4b4b,NAN -    AvgRssi: %u  numSamples=%u [%u %u %u %u %u %u %u %u %u %u %u %u %u %u %u %u ]
56441,I,NAN - CANDIDATE_BEACONS: received %u
56442,2I,NAN - TSF_OFFSET: 0x%08x_%08x
56443,3I,NAN - ANCHORMASTER_RECORD_UPDATE_LAST:  rank=0x%08x_%08x BTT=0x%08x
56444,5I,NAN - ANCHORMASTER_RECORD_EXPIRED2:  rank=0x%08x_%08x HC=%d BTT=0x%08x ==> Setting HC to %u
56445,4I,NAN - BEACON_TX_SEND: type 0x%X  tsfLo 0x%08x  rval %u  hc %u
56446,I,NAN - BEACON_TX_CANCEL: tsfLo 0x%08x
56447,4I,NAN - NAN_SCAN_EVENT: scan_id %u  etype %u  ereason %u  freq %u
56448,I,NAN_DBGID_NAN_SDF_QUEUED : sdf_queued = %d
56449,I,NAN_DBGID_NAN_BEACON_QUEUED : bcn_queued = %d
56450,,WLAN_MODULE_NAN_MODULE_ID - NAN_DBGID_END
56832,,IBSS_PWRSAVE -  IBSS_PS_DBGID_DEFINITION_START 
56833,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PEER_CREATE  IBSS PS: create peer ID=%u
56834,4I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PEER_DELETE  IBSS PS: delete peer ID=%u num_peers:%d num_sleeping_peers:%d ps_enabled_for_this_peer:%d
56835,,IBSS_PWRSAVE -  IBSS_PS_DBGID_VDEV_CREATE  IBSS PS: vdev created
56836,,IBSS_PWRSAVE -  IBSS_PS_DBGID_VDEV_DELETE IBSS PS: vdev deleted
56837,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_VDEV_EVENT  IBSS PS: vdev event:%0x
56838,4I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PEER_EVENT  IBSS PS: Peer event:%0x for peer:%0x sm_event_mask:%0x peer_type:%0x
56839,4I,IBSS_PWRSAVE -  IBSS_PS_DBGID_DELIVER_CAB  IBSS PS: Deliver CAB n_mpdu:%d send_flags:%0x tid_cur:%d q_depth_for_other_tid:%d
56840,4I,IBSS_PWRSAVE -  IBSS_PS_DBGID_DELIVER_UC_DATA  IBSS PS: Deliver data peer:%d tid:%d n_mpdu:%d send_flags:%0x
56841,4I,IBSS_PWRSAVE -  IBSS_PS_DBGID_DELIVER_UC_DATA_ERROR  IBSS PS: Deliver data error peer:%d tid:%d allowed_tidmask:%0x  pending_tidmap:%0x
56842,2I,IBSS_PWRSAVE -  IBSS_PS_DBGID_UC_INACTIVITY_TMR_RESTART  IBSS PS: UC timer restart peer:%d timer_val:%0x
56843,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_MC_INACTIVITY_TMR_RESTART  IBSS PS: MC timer restart timer_val:%0x
56844,3I,IBSS_PWRSAVE -  IBSS_PS_DBGID_NULL_TX_COMPLETION  IBSS PS: null tx completion peer:%d tx_completion_status:%d flags:%0x
56845,4I,IBSS_PWRSAVE -  IBSS_PS_DBGID_ATIM_TIMER_START  IBSS PS: ATIM timer start tsf:%0x %0x tbtt:%0x %0x
56846,2I,IBSS_PWRSAVE -  IBSS_PS_DBGID_UC_ATIM_SEND  IBSS PS: %d Send ATIM to peer:%d
56847,2I,IBSS_PWRSAVE -  IBSS_PS_DBGID_BC_ATIM_SEND  IBSS PS: MC Data  num_of_peers:%d bc_atim_sent:%d
56848,2I,IBSS_PWRSAVE -  IBSS_PS_DBGID_UC_TIMEOUT  IBSS PS: UC timeout for peer:%d send_null:%d
56849,,IBSS_PWRSAVE -  IBSS_PS_DBGID_PWR_COLLAPSE_ALLOWED IBSS PS: allow power collapse
56850,,IBSS_PWRSAVE -  IBSS_PS_DBGID_PWR_COLLAPSE_NOT_ALLOWED  IBSS PS: power collapse not allowed by INI
56851,2I,IBSS_PWRSAVE -  IBSS_PS_DBGID_SET_PARAM  IBSS PS: Set Param ID:%0x Value:%0x
56852,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_HOST_TX_PAUSE  IBSS PS: Pausing host  vdev_map:%0x
56853,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_HOST_TX_UNPAUSE  IBSS PS: Unpausing host  vdev_map:%0x
56854,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PS_DESC_BIN_HWM  IBSS PS: HWM  vdev_map:%0x
56855,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PS_DESC_BIN_LWM  IBSS PS: LWM  vdev_map:%0x
56856,3I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PS_KICKOUT_PEER  IBSS PS: Kickout peer id:%d atim_fail_cnt:%d status:%d
56857,3I,IBSS_PWRSAVE -  IBSS_PS_DBGID_SET_PEER_PARAM  IBSS PS: Set Peer Id:%d Param ID:%0x Value:%0x
56858,4I,IBSS_PWRSAVE -  IBSS_PS_DBGID_BCN_ATIM_WIN_MISMATCH  IBSS PS: %d ATIM window length mismatch  our's:%d  peer id:%d  peer's:%d
56859,2I,IBSS_PWRSAVE -  IBSS_PS_DBGID_RX_CHAINMASK_CHANGE  IBSS PS: Chainmask change current:%0x  Vote for low pwr chainmask:%d
56860,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_BT_STATE_CHANGE  IBSS PS: BT State:%d
56861,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_SELF_PS_STATE_NOTIFICATION_TMR_RESTART  IBSS PS: Self PS state notification timer expired  timeout value:%0x
56862,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PEER_PS_STATE_MONITOR_TMR_EXPIRED  IBSS PS: Peer PS state monitor timer expired  timeout value:%0x
56863,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PEER_CREATION_FAILURE  IBSS PS: peer alloc failed for peer ID:%u
56864,,IBSS_PWRSAVE -  IBSS_PS_DBGID_VDEV_CREATION_FAILURE  IBSS PS: vdev alloc failed
56865,,IBSS_PWRSAVE -  IBSS_PS_DBGID_UC_ATIM_SEND_NO_PEERS  IBSS PS: no peers to send UC ATIM
56866,3I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PEER_ATIM_WIN_MISMATCH  IBSS PS: Peer ATIM window length changed  peer id:%d  peer recorded atim window:%d new atim window:%d
56867,,IBSS_PWRSAVE -  IBSS_PS_DBGID_PWR_COLLAPSE_NOT_ALLOWED_ZERO_PEERS  IBSS PS: power collapse not allowed - no peers in NW 
56868,2I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PWR_COLLAPSE_NOT_ALLOWED_NON_EMPTY_QUEUES  IBSS PS: power collapse not allowed  non-zero qdepth %d %d
56869,I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PWR_COLLAPSE_NOT_ALLOWED_PEER_PS_DISABLED  IBSS PS: power collapse not allowed since peer id:%d is not PS capable
56870,2I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PWR_COLLAPSE_NOT_ALLOWED_PEER_PS_STATE_MC  IBSS PS: power collapse not allowed by peer:%d peer_flags:%0x
56871,4I,IBSS_PWRSAVE -  IBSS_PS_DBGID_PWR_COLLAPSE_NOT_ALLOWED_IBSS_PS_STATE_MC  IBSS PS: power collapse not allowed by state m/c nw_cur_state:%d nw_next_state:%d ps_cur_state:%d flags:%0x
57344,,WLAN_MODULE_HIF_UART
57345,2I,HIF_UART -  Fatal (%d) - WAKE-ACK timeout in %d ms
57346,I,HIF_UART -  Fatal (%d) - TX failed
57347,I,HIF_UART -  Fatal (%d) - Out of RX free HTC buffer
57348,I,HIF_UART -  Fatal (%d) - Unknown
57349,2I,HIF_UART -  Current power state RX(%d),TX(%d): 1-RX/TX-Wake,2-TX-Wake-Pending,4-RX/TX-Sleep
57350,3I,HIF_UART -  With event (%d), transit power state toRx(%d),Tx(%d): 1-TX-pause,2-TX-resume,3-RXedWake,4-RxedWakeAck,5-WakeAckTimeout,6-RxedSleep
57351,,HIF_UART -  TX/RX both idle. Putting UART SLEEP
57352,,HIF_UART -  Out of RX free HTC buffer. WMI svc not provide.
57353,,HIF_UART -  RX: Just return from Rx state macine. defer timer has been started already
57354,I,HIF_UART -  RX: Reach to MAX RX recursion (%d)
57355,3I,HIF_UART -  RX: Received - 1st byte(0x%x) in length(%d), more(%d)
57356,,HIF_UART -  RX: Sent XON
57357,I,HIF_UART -  RX: Return HTC buffer with actual_length(%d) to WMI svc
57358,I,HIF_UART -  RX: CRC error and drop the buffer with length(%d), dump buffer in VERBOSE level
57359,I,HIF_UART -  RX: 0x%x
57360,,HIF_UART -  TX: Just return from Tx state macine. defer timer has been started already
57361,I,HIF_UART -  TX: Reach to MAX TX recursion (%d)
57362,I,HIF_UART -  TX: Buffer overflow after HDLC - payload length(%d), Will drop the packet
57363,3I,HIF_UART -  TX: not enough room in UART ring avail(%d)/required(%d), will retry in %d ms
57364,2I,HIF_UART -  TX: Fail to send %d of %d bytes. Will retry entire payload in 2 ms
57365,2I,HIF_UART -  TX: Successfully sent %d bytes. %d remains
57366,I,HIF_UART -  TX: Successfully sent %d bytes.
57367,,HIF_UART -  RX: Wake UP!
57368,,HIF_UART -  Geofencing / LPASS interface is disabled
57369,,HIF_UART -  Geofencing / LPASS interface is enabled
57370,,WLAN_MODULE_HIF_UART -  TX: Try to sleep
57856,,WLAN_MODULE_LPI
57857,2I,LPI: _wlan_lpi_scan_evt_handler : %d evt_type:0x%x
57858,3I,LPI: _wlan_lpi_scan_evt_handler snoop scan : %d chan_freq:%d num_chan_scaned:%d
57859,I,LPI: _wlan_lpi_update_age_of_measurement : %d
57860,2I,LPI: _wlan_lpi_check_if_entry_present : mac: %x:%x
57861,2I,LPI: wmi_lpi_complete : %d tx_cmpl_counter : %d
57862,I,LPI: _wlan_lpi_send_result : %d
57863,I,LPI: _wlan_lpi_send_result : Sending Scan results to ADSP send_counter : %d
57864,4I,LPI: _wlan_lpi_send_result : %d data_len:%d len_of_chan_scaned: %d, total:%d
57865,3I,LPI: _wlan_lpi_send_result : %d RESULT_DATA_SIZE:%d total:%d
57866,2I,LPI: _wlan_lpi_send_status_event : %d status:0x%x
57867,I,LPI: _wlan_lpi_send_handoff_event : %d
57868,3I,LPI: _wlan_lpi_send_handoff_event : %d ctxt-ssid_len:%d resp:ssid_len:%d
57869,4I,LPI: _wlan_lpi_send_handoff_event : %d freq:%d rssi:%d vdev_id:%d
57870,2I,LPI: _wlan_lpi_probe_rsp_beacon_handler : %d ie_bitmap:0x%x
57871,2I,LPI: _wlan_lpi_probe_rsp_beacon_handler : %d ie_bitmap:0x%x
57872,6I,LPI: _wlan_lpi_probe_rsp_beacon_handler : mac : %02X:%02X:%02X:%02X:%02X:%02X
57873,2I,LPI: _wlan_lpi_probe_rsp_beacon_handler : %d is_probe:%d
57874,2I,LPI: _wlan_lpi_probe_rsp_beacon_handler : %d freq:%d
57875,2I,LPI: _wlan_lpi_probe_rsp_beacon_handler : %d data_buff_index:%d
57876,2I,LPI: _wlan_wmi_lpi_mgmt_snooping_config : %d enable:%d
57877,I,LPI: _wlan_wmi_lpi_scan_start : %d
57878,3I,LPI: _wlan_wmi_lpi_scan_start : %d scan_req_id:%d scan_id:%d
57879,2I,LPI: _wlan_wmi_lpi_scan_start - WMI_LPI_STATUS_ILLEGAL_CHAN_REQ %d num_chan:%d
57880,2I,LPI: _wlan_wmi_lpi_scan_start - WMI_LPI_STATUS_DROPPED_REQ %d num_ssids:%d
57881,2I,LPI: _wlan_wmi_lpi_scan_start - WMI_LPI_STATUS_DROPPED_REQ %d num_bssid:%d
57882,2I,LPI: _wlan_wmi_lpi_scan_start - WMI_LPI_STATUS_DROPPED_REQ %d ie_len:%d
57883,I,LPI: _wlan_wmi_lpi_scan_stop %d
57884,I,LPI: _wlan_wmi_lpi_scan_stop %d status:0x%x
57885,I,LPI: _wlan_lpi_handoff_handler %d
57886,I,LPI: _wlan_lpi_init %d
57887,I,LPI: _wlan_lpi_register %d
57888,3I,LPI: _wlan_lpi_send_result - !! Never reach here: %d data_size:%d Event_size:%d
57889,3I,LPI: _wlan_lpi_scan_evt_handler Discovery scan : %d chan_freq:%d num_chan_scaned:%d
57890,2I,LPI: _wlan_lpi_send_result : %d num_chan_scaned:%d
57891,I,LPI: _wlan_lpi_send_result : %d Send In Progress not got wmi_lpi_complete cb yet !!!
57892,5I,LPI: _wlan_wmi_lpi_scan_start : %d dw_act:%d dw_pas:%d min_rest:%d max_rest:%d
57893,5I,LPI: _wlan_wmi_lpi_scan_start : %d r_prob:%d spc_prob:%d idle_t:%d max_scn_time:%d
57894,5I,LPI: _wlan_wmi_lpi_scan_start : prob_dly:%d burst_durat:%d priority:%d vdev_id:%d ctrl_flag:0x%x
57895,4I,LPI: _wlan_wmi_lpi_scan_start : n_chan:%d n_ssids:%d n_bssid:%d ie_len:%d
57896,2I,LPI: _wlan_lpi_probe_rsp_beacon_handler : mac: %x:%x
57897,2I,LPI: _wlan_wmi_lpi_scan_start : %d Magic frequency:%d GHz Send from ADSP to check current firmware status(Is responsive) 
58368,,WLAN_MODULE_EXTSCAN -  EXTSCAN_START
58369,5I,EXTSCAN -  EXTSCAN_STOP  request_id = %u requestor_id = %u vdev_id = %u table_id = %u vdev_id = %u
58370,5I,EXTSCAN -  EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x
58371,3I,EXTSCAN -  EXTSCAN_GET_FREE_ENTRY_SUCCESS  address of first free bssid entry = 0x%x bssid table free entry count = %u bssid addr 0x%x
58372,2I,EXTSCAN -  EXTSCAN_GET_FREE_ENTRY_INCONSISTENT  bssid table free entry count = %u address of first free bssid entry 0x%x
58373,I,EXTSCAN -  EXTSCAN_GET_FREE_ENTRY_NO_MORE_ENTRIES  address of first free bssid entry = 0x%x
58374,4I,EXTSCAN -  EXTSCAN_CREATE_ENTRY_SUCCESS  compressed mac address 0x%x first free bssid entry addr 0x%x ssid len %u no. if free bssid entries left %u
58375,I,EXTSCAN -  EXTSCAN_CREATE_ENTRY_ERROR  arg1 = 0x%x
58376,5I,EXTSCAN -  EXTSCAN_SEARCH_SCAN_ENTRY_QUEUE  rx frame addr 3 = 0x%x 0x%x 0x%x 0x%x 0x%x
58377,2I,EXTSCAN -  EXTSCAN_SEARCH_SCAN_ENTRY_KEY_FOUND  scan entry reference value = 0x%x compressed mac addr = 0x%x
58378,I,EXTSCAN -  EXTSCAN_SEARCH_SCAN_ENTRY_KEY_NOT_FOUND  compressed mac addr = 0x%x
58379,4I,EXTSCAN -  EXTSCAN_ADD_ENTRY  compressed mac addr = 0x%x scan frame channel = 0x%x scan frame rssi = 0x%x channel match = %u
58380,4I,EXTSCAN -  EXTSCAN_BUCKET_SEND_OPERATION_EVENT  arg1 = 0x%x event_type %u request id %u no of buckets %u
58381,I,EXTSCAN -  EXTSCAN_BUCKET_SEND_OPERATION_EVENT_FAILED  scan start failed event type = 0x%x
58382,4I,EXTSCAN -  EXTSCAN_BUCKET_START_SCAN_CYCLE  arg1 = 0x%x timer tick = %u scheduled_bucket_mask = 0x%x no of buckets = %u
58383,4I,EXTSCAN -  EXTSCAN_BUCKET_PERIODIC_TIMER  arg1 = 0x%x timer running = %u timer tick = %u base period %u
58384,4I,EXTSCAN -  EXTSCAN_SEND_START_STOP_EVENT  command id = %u extscan operation mode = 0x%x send event status = 0x%x request id = %u
58385,,EXTSCAN -  EXTSCAN_NOTIFY_WLAN_CHANGE 
58386,,EXTSCAN -  EXTSCAN_NOTIFY_WLAN_HOTLIST_MATCH 
58387,,EXTSCAN -  EXTSCAN_MAIN_RECEIVED_FRAME 
58388,,EXTSCAN -  EXTSCAN_MAIN_NO_SSID_IE 
58389,I,EXTSCAN -  EXTSCAN_MAIN_MALFORMED_FRAME  invalid ssid length = %u
58390,,EXTSCAN -  EXTSCAN_FIND_BSSID_BY_REFERENCE 
58391,I,EXTSCAN -  EXTSCAN_FIND_BSSID_BY_REFERENCE_ERROR  bssid reference value (hash value + position) = 0x%x
58392,4I,EXTSCAN -  EXTSCAN_NOTIFY_TABLE_USAGE  table_type = %u request id = %u entries in use = %u maximum entries = %u
58393,4I,EXTSCAN -  EXTSCAN_FOUND_RSSI_ENTRY  compressed mac address = 0x%x rssi table entry idx = %u bssid reference value = 0x%x rssi val = %u
58394,4I,EXTSCAN -  EXTSCAN_BSSID_FOUND_RSSI_SAMPLE  compressed mac addr = 0x%x current idx in rssi table = %u rx frame rssi value %u current idx rssi value 0x%x
58395,3I,EXTSCAN -  EXTSCAN_BSSID_ADDED_RSSI_SAMPLE  compressed mac addr = 0x%x no of entries in rssi table = %u max entries in rssi table = %u
58396,4I,EXTSCAN -  EXTSCAN_BSSID_REPLACED_RSSI_SAMPLE  compressed mac addr = 0x%x current idx in rssi table = %u rx frame rssi = %u current idx rssi %u
58397,3I,EXTSCAN -  EXTSCAN_BSSID_TRANSFER_CURRENT_SAMPLES  rssi table current entry count = %u entry count = %u no os rssi samples = %u
58398,4I,EXTSCAN -  EXTSCAN_BUCKET_PROCESS_SCAN_EVENT  scan cycle in progress = %u scan ID = %u scan event type = 0x%x requestor id = %u
58399,5I,EXTSCAN -  EXTSCAN_BUCKET_CANNOT_FIND_BUCKET  arg1 = 0x%x scan cycle in progress = %u scan ID = %u scan event type = 0x%x requestor id = %u
58400,3I,EXTSCAN -  EXTSCAN_START_SCAN_REQUEST_FAILED  bucket index = %u bucket scan id = %u scan events to be notified for bucket = 0x%x
58401,2I,EXTSCAN -  EXTSCAN_BUCKET_STOP_CURRENT_SCANS  scheduled bucket mask = 0x%x is extscan running = %u
58402,3I,EXTSCAN -  EXTSCAN_BUCKET_SCAN_STOP_REQUEST  loop i value = %u bucket id = %u  bucket scan id = %u
58403,,EXTSCAN -  EXTSCAN_BUCKET_PERIODIC_TIMER_ERROR
58404,5I,EXTSCAN -  EXTSCAN_BUCKET_START_OPERATION  request id = %u no of buckets = %u no of channels = %u scan priority = %u is extscan running = %u
58405,3I,EXTSCAN -  EXTSCAN_START_INTERNAL_ERROR  Register event handler for bucket events to host request id = %u requestor id = %u status = %u
58406,2I,EXTSCAN -  EXTSCAN_NOTIFY_HOTLIST_MATCH  compressed mac addr = 0x%x flags = 0x%x
58407,,EXTSCAN -  EXTSCAN_CONFIG_HOTLIST_TABLE 
58408,,EXTSCAN -  EXTSCAN_CONFIG_WLAN_CHANGE_TABLE 
58880,4I,WLAN_MODULE_UNIT_TEST -  UNIT_TEST_GEN  0x%x 0x%x 0x%x 0x%x
59392,5I,WLAN_MODULE_MLME -  MLME_DEBUG_CMN  0x%x 0x%x 0x%x 0x%x 0x%x
59393,,WLAN_MODULE_MLME -  MLME_DEBUG_IF 
59394,,WLAN_MODULE_MLME -  MLME_DEBUG_AUTH 
59395,,WLAN_MODULE_MLME -  MLME_DEBUG_REASSOC 
59396,,WLAN_MODULE_MLME -  MLME_DEBUG_DEAUTH 
59397,,WLAN_MODULE_MLME -  MLME_DEBUG_DISASSOC 
59398,,WLAN_MODULE_MLME -  MLME_DEBUG_ROAM 
59399,,WLAN_MODULE_MLME -  MLME_DEBUG_RETRY 
59400,,WLAN_MODULE_MLME -  MLME_DEBUG_TIMER 
59401,5I,WLAN_MODULE_MLME -  MLME_DEBUG_FRAMEPARSE  0x%x 0x%x 0x%x 0x%x 0x%x
59904,5I,SUPPL -  SUPPL_DBGID_INIT  0x%x 0x%x 0x%x 0x%x 0x%x
59905,3I,SUPPL -  SUPPL_RECV_EAPOL  recv_sz = %d cur_event = 0x%x (RX_M1 0/RX_M2 1/RX_M3 2/RX_M4 3/RX_GM1 4/RX_GM2 5/RX_MICERR 6/TIMEOUT 7/DISC 8/FINISH 9) cur_proto = 0x%x (WPA 1/RSN 2)
59906,3I,SUPPL -  SUPPL_RECV_EAPOL_TIMEOUT  side = %d, cur_state = 0x%x (NULL 0/INIT 1/SENT_M2 2/SENT_M4 3/CONNECTED 4) status = %d (UNDEF 0/SUCC 1/M1_TO 2/M3_TO 3/GM1_TO 4)
59907,3I,SUPPL -  SUPPL_SEND_EAPOL  send_sz = %d cur_event = 0x%x (RX_M1 0/RX_M2 1/RX_M3 2/RX_M4 3/RX_GM1 4/RX_GM2 5/RX_MICERR 6/TIMEOUT 7/DISC 8/FINISH 9) status = 0x%x 
59908,5I,SUPPL -  SUPPL_MIC_MISMATCH  len = %d ucipher = 0x%x pmk_len = %d pmk(first 8 byte) = %08x:%08x
59909,5I,SUPPL -  SUPPL_FINISH status = %d LOW 4 BYTE of peer = %02x:%02x:%02x:%02x  
59910,5I,SUPPL -  SUPPL_GET_FRM_INFO sz = %d, proto = 0x%x key_info = 0x%x keydata_len = %d evt = 0x%x 
59911,2I,SUPPL -  SUPPL_DUMP_TYPE dump_type = %d (PMK 0/MSK 1/KRK 2/BTK 3/R0KH_ID 4/PTK 5/GTK 6) dump_len = %d
59912,5I,SUPPL -  SUPPL_DUMP_HEX index = %d LSB->MSB %08x:%08x:%08x:%08x
59913,4I,SUPPL -  SUPPL_NODE_NOT_FOUND  unique id = 0x%x parameter = 0x%x, SA = %08x:%08x (MSB->LSB) 
59914,3I,SUPPL -  SUPPL_GET_EAPOL_BUF len = %d, remote_addr = 0x%x index = 0x%x (0xbfe4f011 = buffer full)
59915,I,SUPPL - SUPPL_DBGID_GET_BUF_FAIL cur_event = 0x%x  (RX_M1 0/RX_M2 1/RX_M3 2/RX_M4 3/RX_GM1 4/RX_GM2 5/RX_MICERR 6/TIMEOUT 7/DISC 8/FINISH 9)
60416,,WLAN_MODULE_ERE - ERE_DBGID_DEFINITION_START
60417,2I,ERE - ERE_DBGID_VDEV_ATTACH  ere_handle1=0x%x ere_handle2=0x%x
60418,2I,ERE - ERE_DBGID_VDEV_DETACH  ere_handle=0x%x pdev=0x%x
60419,2I,ERE - ERE_DBGID_ENABLE_CMD  mode=0x%x ere_handle=0x%x
60420,I,ERE - ERE_DBGID_STATUS_ENABLED  ere_handle=0x%x
60421,,ERE - ERE_DBGID_STATUS_DISABLED 
60422,4I,ERE - ERE_DBGID_ISROUTE_TABLE_EMPTY status=0x%x ere_handle=0x%x ere_handle_valid=0x%x ere_handle_numEntries=0x%x 
60423,2I,ERE - ERE_DBGID_HASH_VALUE 0x%x uHash=0x%x
60424,5I,ERE - ERE_DBGID_MATCH_REQ uMatchFound=0x%x curIpHash=0x%x mac_addr31to0=0x%x mac_addr32to47=0x%x tblIdx=0x%x
60425,5I,ERE - ERE_DBGID_ADD_ROUTE_DBG idx=0x%x value1=0x%x value2=0x%x value3=0x%x value4=0x%x
60426,5I,ERE - ERE_DBGID_ADD_ROUTE_ENTRY value1=0x%x value2=0x%x value3=0x%x value4=0x%x value5=0x%x
60427,,ERE - ERE_DBGID_STATS_TX 
60428,,ERE - ERE_DBGID_STATS_RX 
60429,,WLAN_MODULE_ERE - ERE_DBGID_DEFINITION_END
60928,, WLAN_MODULE_ID_INVALID
